Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	835	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	23/10/91	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7692556 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	406231  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Mesotrophic Yellow Chromosol Thick Non-	Principal Profile Form:	Dy3.42
	gravelly Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 1.01-3m, Mid-dense. *Species includes - Aristida species, Dichanthium species, 
	Heteropogon contortus	Mid Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus polycarpa, Eucalyptus papuana, Eucalyptus 
	crebra
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Single grain grade of structure; 
	Earthy fabric; Dry; Loose consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 
	0.05); Clear change to - 
	A12	0.08 - 0.18 m	Brown (10YR4/3-Moist); ; Sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Clear change to - 
	A21	0.18 - 0.4 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Loose consistence; , Calcareous, , ; , Gypseous, , ; Diffuse change to - 
	A21c	0.4 - 0.5 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Loose consistence; Many (20 - 50 %), Manganiferous, Coarse (6 - 20 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Abrupt change to - 
	B21	0.5 - 0.6 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR68, 20-50% , 5-15mm, Prominent; Mottles, 
	20-50% ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped
	 fabric; Moderately moist; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	835	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	835	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile