Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	858	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	04/11/91	Elevation:	250 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7715090 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	431316  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Epipedal Grey Vertosol Non-	Principal Profile Form:	Ug5.27
	gravelly Fine Medium fine Very deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida species, Dichanthium species
	Mid Strata - , , . *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Acacia argyrodendron
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Dark greyish brown (2.5Y4/2-Moist); ; Light medium clay; Moderate grade of structure, 10-20 
	mm, Subangular blocky; , Calcareous, , ; , Gypseous, , ; 
	A12	0.02 - 0.3 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Strong grade of structure, 50-100 
	mm, Subangular blocky; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Concretions; , Gypseous, 
	, ; Field pH 9.5 (Raupach, 0.05); 
	B21	0.3 - 0.85 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Moderate grade of structure, 100-
	200 mm, Lenticular; Common cutans, 10-50% of ped faces or walls coated, distinct; Few (2 - 
	10 %), Calcareous, Fine (0 - 2 mm), Concretions; , Gypseous, , ; Field pH 9.5 (Raupach, 0.6); 
	B22	0.85 - 1.5 m	Dark greyish brown (2.5Y4/3-Moist); Mottles, 10YR52, 2-10% , 5-15mm, Distinct; Mottles, 2-
	10% ; Medium heavy clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Few (2 - 
	10 %), Calcareous, Fine (0 - 2 mm), Concretions; , Gypseous, , ; Field pH 9.5 (Raupach, 1.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	858	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.02 - 0.3	8A	16B	7.4	0.22	0.71
	0.3 - 0.85	8.4A	12B	7.6	0.12	6.3	23.1I	27.27
	11.8J	7.6	0.1	3.1	13.42
	0.85 - 1.5	7.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.02 - 0.3
	0.3 - 0.85
	0.85 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.02 - 0.3
	0.3 - 0.85
	0.85 - 1.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	858	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension