Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	864	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	05/11/91	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7729597 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	449667  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Hypernatric Grey Sodosol Medium Slightly gravelly 	Principal Profile Form:	Dy3.11
	Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Soloth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, subrounded, Detrital sedimentary rock (unidentified)
	Profile Morphology
	A1	0 - 0.12 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; ,
	 Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	B21	0.12 - 0.3 m	Grey (10YR5/1-Moist); ; Medium clay; Weak grade of structure, 10-20 mm, Subangular blocky; 
	Smooth-ped fabric; 10-20%, medium gravelly, 6-20mm, subrounded, dispersed, Detrital 
	sedimentary rock (unidentified), coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.2); 
	B22	0.3 - 0.45 m	Greyish brown (10YR5/2-Moist); Mottles, 10YR53, 10-20% , 5-15mm, Distinct; Mottles, 10-20% ;
	 Medium heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped 
	fabric; 2-10%, fine gravelly, 2-6mm, subrounded, dispersed, Detrital sedimentary rock 
	(unidentified), coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	B23	0.45 - 0.6 m	Grey (10YR6/1-Moist); Mottles, 5YR56, 10-20% , 5-15mm, Distinct; Mottles, 10-20% ; Medium 
	heavy clay; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 2-10%,
	 fine gravelly, 2-6mm, subrounded, dispersed, Detrital sedimentary rock (unidentified), coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 5.6 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	864	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	6.3A
	0.12 - 0.3	6.5A	1.3J	10	0.1	5	14I	35.71
	0.45 - 0.6	5.1A	0.7J	5.7	0.1	1.5	8.6I	17.44
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.3
	0.45 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.3
	0.45 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	864	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension