Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	880	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	08/11/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8256   GPS	Rainfall:	No Data
	Northing/Long.:	7723482 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	477824  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Brown Chromosol Medium Non-gravelly Clay-	Principal Profile Form:	Dy3.53
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, angular, Quartz
	Profile Morphology
	A11	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Clay loam, coarse sandy; Massive grade of structure; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear change to - 
	A12	0.1 - 0.15 m	Brown (10YR4/3-Moist); ; Clay loam, coarse sandy (Heavy); Massive grade of structure; , 
	Calcareous, , ; , Gypseous, , ; Clear change to - 
	B21	0.15 - 0.45 m	Yellowish brown (10YR5/8-Moist); ; Medium clay; Weak grade of structure, 10-20 mm, 
	Subangular blocky; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.3); Clear change to - 
	B22	0.45 - 0.9 m	Yellowish brown (10YR5/8-Moist); Mottles, 2.5YR48, 10-20% , 5-15mm, Distinct; Mottles, 10-
	20% ; Light medium clay; Weak grade of structure, 10-20 mm, Subangular blocky; Common (10 -
	 20 %), Manganiferous, Medium (2 -6 mm), Veins; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 
	(Raupach, 0.6); Gradual change to - 
	B3	0.9 - 1.5 m	Dark red (2.5YR3/6-Moist); Mottles, 10YR66, 2-10% , 0-5mm, Prominent; Mottles, 2-10% ; Light 
	medium clay; Weak grade of structure, 10-20 mm, Subangular blocky; 2-10%, medium gravelly, 
	6-20mm, angular, dispersed, Metamorphic rock (unidentified), coarse fragments; Common (10 - 
	20 %), Manganiferous, Medium (2 -6 mm), Veins; , Calcareous, , ; , Gypseous, , ; Field pH 8 
	(Raupach, 1.3); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	880	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7A
	0.15 - 0.45	7A	3.9J	1.1	0	0.2	5.2I	3.85
	0.9 - 1.5	6.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.15 - 0.45
	0.9 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.15 - 0.45
	0.9 - 1.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	880	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension