Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	886	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	19/11/91	Elevation:	270 metres
	Map Ref.:	Sheet No. : 8256   GPS	Rainfall:	No Data
	Northing/Long.:	7701004 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	460076  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Grey Sodosol Very thick Non-gravelly 	Principal Profile Form:	Dy4.83
	Sandy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Chloris species, Heteropogon contortus, Aristida 
	species	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Grevillea species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus papuana, Eucalyptus platyphylla
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.08 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.05); 
	A12j	0.08 - 0.28 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; 
	A2e	0.28 - 0.6 m	Light yellowish brown (10YR6/4-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 
	(Raupach, 0.6); 
	B2	0.6 - 0.62 m	Light grey (10YR7/2-Moist); ; Coarse sandy clay loam; Massive grade of structure; Sandy 
	(grains prominent) fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; 
	Silcrete, Moderately cemented, Continuous, Massive; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	886	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	886	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile