Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	9	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	21/06/90	Elevation:	255 metres
	Map Ref.:	Sheet No. : 8258   GPS	Rainfall:	No Data
	Northing/Long.:	7788792 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	468470  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granodiorite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	10 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Thin Non-gravelly Clayey 	Principal Profile Form:	Uf6.34
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Bothriochloa pertusa, Eriachne species
	Mid Strata - , , . *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Reddish brown (5YR4/3-Moist); ; , 0-0% ; Light clay; Strong grade of structure, 2-5 mm, 
	Granular; Smooth-ped fabric; Moist; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH
	 6 (Raupach, 0.05); Common, fine (1-2mm) roots; Gradual, Smooth change to - 
	A3	0.05 - 0.25 m	Reddish brown (5YR4/3-Moist); ; , 0-0% ; Light clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, 
	angular, dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Common, fine (1-
	2mm) roots; Clear, Smooth change to - 
	B2	0.25 - 0.45 m	Red (2.5YR5/8-Moist); ; , 0-0% ; Light medium clay; Moderate grade of structure, 50-100 mm, 
	Angular blocky; Smooth-ped fabric; Moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, 
	angular, dispersed, Substrate material, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field 
	pH 6.8 (Raupach, 0.3); Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	BC	0.45 - 0.53 m	Yellowish red (5YR5/8-Moist); ; , 0-0% ; Light medium clay; Strong grade of structure, 20-50 
	mm, Angular blocky; Smooth-ped fabric; Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, 
	angular, dispersed, Substrate material, coarse fragments; , Calcareous, , ; , Gypseous, , ; Few, 
	very fine (0-1mm) roots; Abrupt, Smooth change to - 
	C	0.53 - 0.7 m	; , 0-0% ; Moderately moist; Weak consistence; 2-10%, fine gravelly, 2-6mm, angular, 
	dispersed, Substrate material, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 
	(Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	9	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	7.5A	6.9B	2.4	0.4	0.05
	0.25 - 0.45	7.9A	13B	3.2	0.17	0.18	22.1I	0.81
	12.1J	3.1	0.1	0	0.00
	0.53 - 0.7	8.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.25 - 0.45
	0.53 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.25 - 0.45
	0.53 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	9	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension