Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	903	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	02/11/91	Elevation:	230 metres
	Map Ref.:	Sheet No. : 8256   GPS	Rainfall:	No Data
	Northing/Long.:	7690488 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	476275  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Alluvial plain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Mottled-Subnatric Black Sodosol Thick Non-	Principal Profile Form:	Dd2.43
	gravelly Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Isolated plants. *Species includes - Cyperus species, Heteropogon contortus
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Acacia harpophylla, Lysiphillum carronii
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.19 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam (Heavy); Massive grade of structure; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.05); 
	A12j	0.19 - 0.22 m	Brown (7.5YR4/2-Moist); ; Sandy loam (Heavy); Massive grade of structure; , Calcareous, , ; , 
	Gypseous, , ; 
	B2e	0.22 - 0.3 m	Brown (7.5YR4/2-Moist); ; Sandy loam (Heavy); Massive grade of structure; 2-10%, cobbly, 
	60-200mm, rounded tabular, Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6.8 (Raupach, 0.3); 
	B2	0.3 - 0.4 m	Dark brown (7.5YR3/2-Moist); Mottles, 7.5R54, 10-20% , Distinct; Mottles, 10-20% ; Sandy 
	medium clay; Moderate grade of structure, 100-200 mm, Columnar; , Calcareous, , ; , Gypseous,
	 , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	903	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	903	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile