Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	904	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	02/11/91	Elevation:	No Data
	Map Ref.:	Sheet No. : 8256   GPS	Rainfall:	No Data
	Northing/Long.:	7692334 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	474712  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Grey Sodosol Medium Non-gravelly 	Principal Profile Form:	Dy2.32
	Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Sparse. *Species includes - TRIODIA SPECIES ?, Heteropogon contortus
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Acacia cambagei
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Brown (10YR4/3-Moist); ; Sandy loam (Heavy); Massive grade of structure; Weak consistence;
	 , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); 
	A12j	0.05 - 0.18 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy clay loam (Heavy); Massive grade of 
	structure; Firm consistence; , Calcareous, , ; , Gypseous, , ; 
	B1j	0.18 - 0.2 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy clay loam (Heavy); Massive grade of 
	structure; Firm consistence; , Calcareous, , ; , Gypseous, , ; 
	B21	0.2 - 0.5 m	Dark greyish brown (10YR4/2-Moist); ; Light medium clay; Strong grade of structure, Prismatic; 
	Strong grade of structure, 5-10 mm, Angular blocky; Very strong consistence; , Calcareous, , ; ,
	 Gypseous, , ; Field pH 8 (Raupach, 0.3); 
	B22	0.5 - 0.8 m	Yellowish brown (10YR5/4-Moist); Mottles, 10YR56, 2-10% , 5-15mm, Distinct; Mottles, 2-10% ;
	 Light medium clay; Moderate grade of structure, Subangular blocky; Very firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	904	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.6A
	0.2 - 0.5	7.6A	7.1J	5.3	0.5	1.2	16.2I	7.41
	0.5 - 0.8	7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.2 - 0.5
	0.5 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.2 - 0.5
	0.5 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	904	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension