Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	908	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	22/04/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7677340 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	440470  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Brown Chromosol Medium Non-gravelly 	Principal Profile Form:	Db2.12
	Silty Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa species, Dichanthium species, Aristida 
	species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus coolibah, Acacia spectabilis
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus coolibah, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Dark brown (7.5YR3/2-Moist); ; Silty loam; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); 
	B1	0.15 - 0.35 m	Brown (7.5YR4/3-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Very firm 
	consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.3); 
	B21	0.35 - 0.6 m	Brown (7.5YR4/4-Moist); Mottles, 2-10% , 0-5mm, Distinct; Mottles, 2-10% ; Light clay; Moderate
	 grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; Dry; Very firm 
	consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.45); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	908	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	908	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile