Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	919	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	23/04/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8256   GPS	Rainfall:	No Data
	Northing/Long.:	7688470 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	449447  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Consolidated rock 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Summit surface	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Reticulate Mesotrophic Brown Chromosol Thick Non-gravelly 	Principal Profile Form:	Dy3.42
	Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Sparse. *Species includes - TRIODIA SPECIES ?
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Melaleuca nervosa, Eucalyptus shirleyi
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus shirleyi, Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Brown (10YR4/3-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); 
	A2c	0.15 - 0.45 m	Light brownish grey (10YR6/2-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; Common (10 - 20 %), Ferruginous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); 
	B2	0.45 - 0.6 m	Yellowish brown (10YR5/6-Moist); Mottles, 10YR62, 2-10% , 15-30mm, Distinct; Mottles, 2-10%
	 ; Medium clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Dry; Strong consistence; Many (20 - 50 %), Ferruginous, Coarse (6 - 20 mm), Concretions; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	919	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	919	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile