Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	92	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	08/08/90	Elevation:	235 metres
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7714568 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	425931  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Very gently sloped
	Slope:	1.5 % 	Aspect:	210 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Dystrophic Red Kandosol Thin Non-gravelly Sandy 	Principal Profile Form:	Gn2.15
	Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	Red earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Eriachne species, Aristida species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus melanophloia, Petalostigma pubescens, Eucalyptus 
	papuana
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus melanophloia, Eucalyptus papuana, Eucalyptus 
	polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark brown (7.5YR3/2-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Many, fine (1-
	2mm) roots; Gradual, Smooth change to - 
	A2	0.08 - 0.15 m	Brown (7.5YR5/4-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Many, fine (1-2mm) roots; Diffuse, Smooth 
	change to - 
	B21	0.15 - 0.45 m	Yellowish red (5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Moderately moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 
	(Raupach, 0.3); Abundant, medium (2-5mm) roots; Diffuse, Smooth change to - 
	B22c	0.45 - 0.75 m	Yellowish red (5YR5/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Moderately moist; Very weak consistence; Many (20 - 50 %), Ferromanganiferous, Coarse (6 - 
	20 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.6); Few, fine (1-
	2mm) roots; Diffuse, Smooth change to - 
	B23cg	0.75 - 1.2 m	Pink (7.5YR7/4-Moist); Mottles, 2.5YR36, 20-50% , 15-30mm, Prominent; Mottles, 20-50% ; 
	Sandy clay loam; Massive grade of structure; Earthy fabric; Moist; Firm consistence; Very many
	 (50 - 100 %), Ferromanganiferous, Very coarse (20 - 60 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.8 (Raupach, 0.9); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	92	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.7A	0.86B	0.36	0.15	0.03
	0.15 - 0.45	5.3A	0.8J	0.3	0.1	0.2	2.6I	7.69
	0.45 - 0.75	5.2A
	0.75 - 1.2	6.4A	0.54B	1.3	0.06	0.06
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.15 - 0.45
	0.45 - 0.75
	0.75 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.15 - 0.45
	0.45 - 0.75
	0.75 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	92	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension