Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	930	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	14/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7702638 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	418844  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Surface flake
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Epipedal Grey Vertosol Non-gravelly Medium 	Principal Profile Form:	Ug5.24
	fine Very fine Very deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Dichanthium sericeum, Bothriochloa species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - , , . *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, subrounded, Quartz
	Profile Morphology
	A11	0 - 0.01 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium clay; Moderate grade of structure, 5-10 mm, 
	Platy; Smooth-ped fabric; Moderately moist; Very weak consistence; Few (2 - 10 %), 
	Calcareous, Coarse (6 - 20 mm), Concretions; , Gypseous, , ; Field pH 9.5 (Raupach, 0.01); 
	A12	0.01 - 0.02 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium clay; Massive grade of structure; Smooth-ped 
	fabric; Moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 
	0.02); 
	A13	0.02 - 0.65 m	Dark greyish brown (2.5Y4/2-Moist); ; Light clay; Strong grade of structure, 20-50 mm, 
	Subangular blocky; Strong grade of structure, 10-20 mm, Subangular blocky; Smooth-ped 
	fabric; Dry; Very strong consistence; Common cutans, 10-50% of ped faces or walls coated; 
	Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, , ; Field pH 9.5
	 (Raupach, 0.5); 
	B21	0.65 - 1.1 m	Very dark greyish brown (2.5Y3/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-
	50 mm, Lenticular; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped 
	fabric; Moderately moist; Very strong consistence; Common cutans, 10-50% of ped faces or 
	walls coated; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, 
	, ; Field pH 9.5 (Raupach, 1); 
	B22	1.1 - 1.7 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 
	mm, Lenticular; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; 
	Moderately moist; Very strong consistence; Common cutans, 10-50% of ped faces or walls 
	coated; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Soft segregations; , Gypseous, , ; Field 
	pH 9.5 (Raupach, 1.5); 
	B23k	1.7 - 2 m	Olive (5Y5/3-Moist); ; Medium heavy clay; Massive grade of structure; Smooth-ped fabric; 
	Moderately moist; Very firm consistence; Many (20 - 50 %), Calcareous, Coarse (6 - 20 mm), 
	Concretions; , Gypseous, , ; Field pH 9.5 (Raupach, 2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	930	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	930	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01	7.3A
	0.65 - 1.1	8.5A
	1.7 - 2	8.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01
	0.65 - 1.1
	1.7 - 2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.65 - 1.1
	1.7 - 2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	930	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension