Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	938	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	15/05/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8156   GPS	Rainfall:	No Data
	Northing/Long.:	7708778 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	415856  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Surface flake
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endocalcareous Epipedal Grey Vertosol Non-gravelly Medium 	Principal Profile Form:	Ug5.24
	fine Very fine Very deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Dichanthium species, Aristida species, Bothriochloa 
	species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark grey (10YR4/1-Moist); ; Light medium clay; Moderate grade of structure, 2-5 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Very weak consistence; 0-2%, fine 
	gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , 
	; Field pH 8 (Raupach, 0.05); 
	A12	0.05 - 0.2 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Moderate grade of structure, 5-10 
	mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Very weak consistence; 0-2%, 
	fine gravelly, 2-6mm, rounded, dispersed, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 9.5 (Raupach, 0.1); 
	B21	0.2 - 0.9 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium heavy clay; Strong grade of structure; Smooth-
	ped fabric; Dry; Strong consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Common cutans, 10-50% of ped faces or walls coated, distinct; Few (2 - 10 
	%), Calcareous, Medium (2 -6 mm), Concretions; , Gypseous, , ; Field pH 9.5 (Raupach, 0.6); 
	B22	0.9 - 1.6 m	Greyish brown (2.5Y5/2-Moist); ; Medium heavy clay; Strong grade of structure; Smooth-ped 
	fabric; Dry; Strong consistence; 2-10%, fine gravelly, 2-6mm, rounded, dispersed, Quartz, 
	coarse fragments; Common cutans, 10-50% of ped faces or walls coated, distinct; Few (2 - 10 
	%), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 
	(Raupach, 1.2); 
	B23	1.6 - 2.5 m	Grey (2.5Y6/1-Moist); Mottles, 7.5YR44, 2-10% , 5-15mm, Prominent; Mottles, 2-10% ; Medium 
	heavy clay; Strong grade of structure; Smooth-ped fabric; Dry; Strong consistence; Common 
	cutans, 10-50% of ped faces or walls coated, distinct; Few (2 - 10 %), Manganiferous, Fine (0 
	- 2 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 5 (Raupach, 2.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	938	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	8.3A
	0.05 - 0.2	8.8A
	0.2 - 0.9	8A
	0.9 - 1.6	5.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.9
	0.9 - 1.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.9
	0.9 - 1.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	938	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension