Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	948	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	01/09/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7770930 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	357635  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cryptogam surface, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Lithic Bleached-Orthic Tenosol Thick Slightly gravelly 	Principal Profile Form:	Uc2.21
	Sandy Sandy Moderately deep
	ASC Confidence:	Great Soil Group:	Siliceous sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Eriachne species, Heteropogon contortus
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus peltata, Melaleuca nervosa
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus peltata, Eucalyptus crebra, Eucalyptus polycarpa
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; 10-20%, fine gravelly, 2-6mm, subrounded, 
	Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear 
	change to - 
	A2e	0.1 - 0.47 m	Yellowish brown (10YR5/4-Moist); ; Loamy sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Dry; Very weak consistence; 10-20%, fine gravelly, 2-6mm, 
	subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 
	0.4); Gradual change to - 
	B2	0.47 - 0.7 m	Yellowish brown (10YR5/6-Moist); ; Clayey sand; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Dry; Very weak consistence; 20-50%, medium gravelly, 6-20mm, 
	subrounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	948	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.7A
	0.47 - 0.7	5.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.47 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.47 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	948	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension