Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	956	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	02/09/92	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7752182 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	359470  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Poached
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Eutrophic Brown Chromosol Thick Non-	Principal Profile Form:	Db1.43
	gravelly Silty Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Sparse. *Species includes - None recorded
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eremophila mitchellii, Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Silty light clay; Massive grade of structure; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Gradual change to - 
	A2e	0.1 - 0.3 m	Greyish brown (10YR5/2-Moist); ; Silty clay loam; Massive grade of structure; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.2); Abrupt change to - 
	B21	0.3 - 0.6 m	Brown (10YR4/3-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Dry; Very strong consistence; Very few (0 - 2 %), Manganiferous, Medium (2 -6 mm), 
	Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.5); 
	B22	0.6 - 0.7 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9 
	(Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	956	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1A
	0.3 - 0.6	6.3A
	0.6 - 0.7	7.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.3 - 0.6
	0.6 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.3 - 0.6
	0.6 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	956	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension