Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	960	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	02/09/92	Elevation:	360 metres
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7735430 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	356363  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting, Poached
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Eutrophic Grey Kandosol Medium Non-gravelly 	Principal Profile Form:	Uf3
	Clayey Clayey Deep
	ASC Confidence:	Great Soil Group:	Grey clay
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Bothriochloa decipiens, 
	Digitaria species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eremophila mitchellii, Eucalyptus brownii, Atalaya hemiglauca
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus papuana, Eucalyptus polycarpa
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, angular, Quartz
	Profile Morphology
	A1	0 - 0.12 m	Very dark grey (10YR3/1-Moist); ; Light medium clay; Massive grade of structure; Earthy fabric;
	 Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.05); 
	Clear change to - 
	A2j	0.12 - 0.22 m	Dark grey (10YR4/1-Moist); ; Light medium clay; Massive grade of structure; Earthy fabric; Dry; 
	Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.2); Abrupt 
	change to - 
	B21	0.22 - 1 m	Dark grey (10YR4/1-Moist); ; Medium heavy clay; Weak grade of structure, 20-50 mm, 
	Polyhedral; Smooth-ped fabric; Moderately moist; Very strong consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 9.5 (Raupach, 0.9); Gradual change to - 
	B22	1 - 1.5 m	Grey (10YR5/1-Moist); ; Sandy medium heavy clay; Massive grade of structure; Earthy fabric; 
	Moderately moist; Strong consistence; 2-10%, fine gravelly, 2-6mm, subangular, Quartz, coarse
	 fragments; Very few (0 - 2 %), Calcareous, Medium (2 -6 mm), Soft segregations; , Gypseous,
	 , ; Soil matrix is Highly calcareous; Field pH 9.5 (Raupach, 1.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	960	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	5.9A
	0.22 - 1	8A
	1 - 1.5	9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.22 - 1
	1 - 1.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.22 - 1
	1 - 1.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	960	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension