Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	965	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	03/09/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 7957   GPS	Rainfall:	No Data
	Northing/Long.:	7766857 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	322822  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	6 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Bleached-Leptic Tenosol Very thick Non-	Principal Profile Form:	Uc2
	gravelly Sandy Sandy Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Heteropogon contortus, Eriachne species, Aristida 
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Acacia species, Petalostigma pubescens, Eucalyptus species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus polycarpa, Eucalyptus crebra
	Surface Coarse Fragments:	2-10%, fine gravelly, 2-6mm, subangular, Quartz
	Profile Morphology
	A1	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Single grain grade of structure; 
	Sandy (grains prominent) fabric; 10-20%, medium gravelly, 6-20mm, subangular, dispersed, 
	Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	A2	0.1 - 0.25 m	Dark brown (10YR3/3-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; 10-20%, medium gravelly, 6-20mm, subangular, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.2); 
	A2e	0.25 - 0.7 m	Light grey (10YR7/2-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; 20-50%, medium gravelly, 6-20mm, subangular, dispersed, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.6); 
	A3	0.7 - 0.8 m	Light brownish grey (10YR6/2-Moist); ; Loamy sand; Massive grade of structure; 50-90%, 
	medium gravelly, 6-20mm, subangular, dispersed, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7.5 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	965	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.5A
	0.1 - 0.25	6.6A
	0.25 - 0.7	6.6A
	0.7 - 0.8	6.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.7
	0.7 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.25
	0.25 - 0.7
	0.7 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	965	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension