Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	972	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	04/09/92	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7744160 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	383509  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Mesotrophic Brown Kandosol Medium Non-	Principal Profile Form:	Gn2.94
	gravelly Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Grey earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Dichanthium sericeum, Chrysopogon fallax, Cyperus 
	species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus brownii, Acacia nervosa
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus papuana, Eucalyptus platyphylla
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam, sandy; Massive grade of structure; 
	Earthy fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 
	0.05); Clear change to - 
	A21j	0.12 - 0.3 m	Brown (10YR5/3-Moist); Mottles, 10YR46, 0-2% , 5-15mm, Distinct; Mottles, 0-2% ; Sandy light 
	clay; Massive grade of structure; Earthy fabric; Dry; Weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 5 (Raupach, 0.2); Gradual change to - 
	A22e	0.3 - 0.6 m	Light brownish grey (10YR6/2-Moist); Mottles, 10YR56, 0-2% , 5-15mm, Distinct; Mottles, 0-2% ;
	 Sandy light clay (Light); Massive grade of structure; Earthy fabric; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.5); Abrupt change to - 
	B21	0.6 - 0.8 m	Brown (10YR5/3-Moist); Mottles, 10YR58, 20-50% , 5-15mm, Distinct; Mottles, 20-50% ; Sandy 
	light clay (Heavy); Weak grade of structure, 10-20 mm, Polyhedral; Earthy fabric; Dry; Very firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	972	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	5.4A
	0.12 - 0.3	5.2A
	0.3 - 0.6	5.7A
	0.6 - 0.8	5.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.3
	0.3 - 0.6
	0.6 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	972	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension