Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	99	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	09/08/90	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8054   GPS	Rainfall:	No Data
	Northing/Long.:	7593538 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	389848  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mottled-Subnatric Yellow Sodosol Medium Non-gravelly	Principal Profile Form:	Dy3.32
	 Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Very sparse. *Species includes - Chrysopogon fallax, Eragrostis species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eremophila mitchellii, Eucalyptus brownii, Acacia species
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; Moderate grade of structure, 5-10 mm, 
	Platy; Smooth-ped fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Few, very fine 
	(0-1mm) roots; Abrupt, Smooth change to - 
	A12	0.02 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Few, very 
	fine (0-1mm) roots; Clear, Smooth change to - 
	A2j	0.05 - 0.25 m	Yellowish brown (10YR5/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Few, very fine (0-1mm) roots; Clear, 
	Smooth change to - 
	B1c	0.25 - 0.55 m	Brownish yellow (10YR6/6-Moist); ; Clay loam, sandy; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; Common (10 - 20 
	%), Ferromanganiferous, Coarse (6 - 20 mm), Concretions; , Calcareous, , ; , Gypseous, , ; Field
	 pH 6.5 (Raupach, 0.3); Diffuse, Smooth change to - 
	B21c	0.55 - 0.95 m	Olive yellow (2.5Y6/6-Moist); Mottles, 2.5Y78, 20-50% , 0-5mm, Faint; Mottles, 20-50% ; Medium
	 clay; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Moderately 
	moist; Firm consistence; Many (20 - 50 %), Ferromanganiferous, Coarse (6 - 20 mm), 
	Concretions; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	99	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.02 - 0.05	6.2A	1.8B	0.84	0.26	0.07
	0.25 - 0.55	6.2A
	0.55 - 0.95	6.9A	1.7B	1.6	0.31	0.14	5.3I	2.64
	1.7J	1.5	0.3	0.3	5.66
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.02 - 0.05
	0.25 - 0.55
	0.55 - 0.95
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.02 - 0.05
	0.25 - 0.55
	0.55 - 0.95

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	99	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension