Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	997	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	16/09/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7756266 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	357953  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Petroferric Yellow Chromosol Medium Non-gravelly 	Principal Profile Form:	Dy2.51
	Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Isolated plants. *Species includes - Heteropogon contortus
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Acacia nervosa, Petalostigma pubescens
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa, Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.07 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	A12	0.07 - 0.2 m	Brown (10YR4/3-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.15); 
	B2	0.2 - 0.6 m	Brownish yellow (10YR6/8-Moist); ; Coarse sandy light clay; Massive grade of structure; 
	Earthy fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	997	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	6.7A
	0.07 - 0.2	6.1A
	0.2 - 0.6	5.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07
	0.07 - 0.2
	0.2 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.2
	0.2 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	997	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension