Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	998	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	16/09/92	Elevation:	No Data
	Map Ref.:	Sheet No. : 8057   GPS	Rainfall:	No Data
	Northing/Long.:	7754106 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	353742  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Grey Kandosol Medium Non-gravelly 	Principal Profile Form:	Gn1.83
	Loamy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Sparse. *Species includes - Bothriochloa species, Cynodon dactylon
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus platyphylla, Eucalyptus polycarpa
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus platyphylla, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Loam; Massive grade of structure; Earthy fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	B11	0.1 - 0.15 m	Dark greyish brown (10YR4/2-Moist); ; Clay loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.15); 
	B22	0.15 - 0.3 m	Reddish brown (2.5YR5/3-Moist); ; Clay loam, sandy; Massive grade of structure; Sandy 
	(grains prominent) fabric; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 0.3); 
	B23	0.3 - 0.5 m	Light yellowish brown (10YR6/4-Moist); ; Fine sandy clay loam; Sandy (grains prominent) 
	fabric; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	998	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.4A
	0.1 - 0.15	7.3A
	0.15 - 0.6	8.7A
	0.3 - 0.5	9.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.6
	0.3 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.15
	0.15 - 0.6
	0.3 - 0.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	998	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension