Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T519	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	05/12/91	Elevation:	277 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7769968 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	449382  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	O-Dr	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	2 % 	Aspect:	320 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Black Dermosol Thin Non-gravelly Loamy 	Principal Profile Form:	Dd2.13
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	All necessary analytical data are available.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - Bothriochloa pertusa, Bothriochloa ewartiana, 
	Chrysopogon fallax	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Dark brown (7.5YR3/3-Moist); ; Sandy loam; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.01); Few, very fine (0-1mm) roots; Sharp, Smooth change to - 
	A/B	0.02 - 0.1 m	Dark brown (7.5YR3/2-Moist); ; Fine sandy clay loam; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Moderate grade of structure, 10-20 mm, Subangular blocky; Earthy fabric; 
	Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.07); 
	Many, very fine (0-1mm) roots; Clear, Wavy change to - 
	B21	0.1 - 0.25 m	Dark brown (7.5YR3/2-Moist); Mottles, 5YR46, 2-10% , 0-5mm, Distinct; Mottles, 2-10% ; Light 
	clay; Strong grade of structure, 20-50 mm, Subangular blocky; Strong grade of structure, 10-20
	 mm, Subangular blocky; Smooth-ped fabric; Dry; Very strong consistence; Common cutans, 
	10-50% of ped faces or walls coated, distinct; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.18); Common, very fine (0-1mm) roots; Clear, Wavy change to - 
	B22	0.25 - 0.38 m	Dark red (2.5YR3/6-Moist); ; Light clay; Massive grade of structure; Smooth-ped fabric; 
	Moderately moist; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach,
	 0.3); Common, very fine (0-1mm) roots; Abrupt, Wavy change to - 
	BC	0.38 - 0.58 m	; Weak grade of structure, 50-100 mm, Angular blocky; Sandy (grains prominent) fabric; Dry; 
	Firm consistence; 2-10%, medium gravelly, 6-20mm, angular, dispersed, Granodiorite, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.5); Few, very fine (0-1mm) 
	roots; Gradual, Wavy change to - 
	C	0.58 - 1 m	; Sandy (grains prominent) fabric; Dry; Weak consistence; 10-20%, medium gravelly, 6-20mm, 
	angular, dispersed, Granodiorite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 8.5
	 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	DLR1025; A11 HORIZON IS SURFACE WASH/OTHER GRASSES HECO1.

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T519	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T519	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	6.67A	0.04A	5.3B	3	0.87	0.13	7.2I	1.81
	5.99J	2.74	0.32	0.02	0.28
	0.02 - 0.1	6.92A	0.04A	11B	5.3	0.8	0.18	17.1I	1.05
	11.3J	4.64	0.23	0.03	0.18
	0.1 - 0.25	7.14A	0.03A
	0.25 - 0.38	7.41A	0.02A	16.7J	6.71	0.06	0.05	18.9D	0.26
	26I	0.19
	0.38 - 0.58	7.86A	0.02A	17B	0.45	0.45	0.42
	0.58 - 1	8.1A	0.02A	7.46J	2.38	0.05	0.04	8.7I	0.46
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	1.8B	0.023A	0.07A	0.808A	50A	33	5	12
	0.02 - 0.1	0.1A	0.6A	0.025A	0.07A	0.964A	37A	28	8	26
	1.7B
	0.1 - 0.25
	0.25 - 0.38	29A	23	10	38
	0.38 - 0.58
	0.58 - 1	65A	21	5	9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.1
	0.1 - 0.25
	0.25 - 0.38
	0.38 - 0.58
	0.58 - 1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T519	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D2_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; automatic extractor
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	17A1	Total potassium - X-ray fluorescence
	19A1	Carbonates - rapid titration
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1	Organic carbon - Walkley and Black
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method