Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T554	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	05/03/92	Elevation:	372 metres
	Map Ref.:	Sheet No. : 8256   GPS	Rainfall:	No Data
	Northing/Long.:	7684794 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	466645  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Clh	Substrate Material:	Undisturbed soil core, 0.6 m 
	deep,Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	5 m,90 m;
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Brown Chromosol Thick Slightly gravelly 	Principal Profile Form:	Dy3.72
	Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Bothriochloa species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Albizia basaltica
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	0-2%, cobbly, 60-200mm, subangular platy, Sandstone
	Profile Morphology
	A11	0 - 0.05 m	Brown (10YR4/3-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Moderately 
	moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.02); 
	Few, fine (1-2mm) roots; Clear, Wavy change to - 
	A21	0.05 - 0.2 m	Yellowish brown (10YR5/6-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; 
	Moderately moist; Very weak consistence; 10-20%, fine gravelly, 2-6mm, rounded, dispersed, 
	Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.1); 
	Common, fine (1-2mm) roots; Gradual, Wavy change to - 
	A22j	0.2 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; 
	Moderately moist; Very weak consistence; 20-50%, medium gravelly, 6-20mm, rounded, 
	dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.25); Common, fine (1-2mm) roots; Clear change to - 
	B1	0.3 - 0.4 m	Light olive brown (2.5Y5/4-Moist); ; Sandy clay loam (Light); Massive grade of structure; Earthy
	 fabric; Dry; Weak consistence; 50-90%, medium gravelly, 6-20mm, subangular platy, 
	dispersed, Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.8 
	(Raupach, 0.35); Few, fine (1-2mm) roots; Clear change to - 
	B2	0.4 - 0.64 m	Olive yellow (2.5Y6/6-Moist); Mottles, 10YR68, 10-20% , 0-5mm, Distinct; Mottles, 2.5YR48, 10-
	20% ; Light medium clay; Massive grade of structure; Earthy fabric; Dry; Firm consistence; 50-
	90%, medium gravelly, 6-20mm, subangular platy, reoriented, Sandstone, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	DLR1060;B HORIZON DISPERSES IN WATER;
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T554	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.95A	0.04A	3.5B	1.3	0.72	0.11	6.7I	1.64
	3.33J	1.13	0.25	0.02	0.30
	0.05 - 0.2	6.66A	0.01A	0.97J	0.66	0.11	0.02	3.9I	0.51
	0.2 - 0.3	6.6A	0.01A
	0.3 - 0.4	7.07A	0.02A
	0.4 - 0.64	7.36A	0.02A	4.1B	7.6	0.8	0.45	16.1D	2.80
	3.71J	7.45	0.07	0.22	13.6I	3.31
	1.37
	1.62
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	1.2B	0.019A	0.06A	0.422A	42A	42	9	7
	0.05 - 0.2	0.4B	42A	45	6	7
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.64	0.016A	1.84A	14A	30	8	47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.64

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T554	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D2_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; automatic extractor
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method