Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T570	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	28/06/93	Elevation:	360 metres
	Map Ref.:	Sheet No. : 8159   GPS	Rainfall:	No Data
	Northing/Long.:	7851966 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	437882  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Summit surface	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol Medium Non-gravelly 	Principal Profile Form:	Dy2.22
	Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Heteropogon contortus, Bothriochloa species
	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus drepanophylla
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus drepanophylla
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, angular, Granite
	Profile Morphology
	A11	0 - 0.03 m	Very dark grey (10YR3/1-Moist); ; Coarse sandy loam (Light); Massive grade of structure; 
	Earthy fabric; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.02); Clear, Smooth change
	A21	0.03 - 0.11 m	Brown (10YR4/3-Moist); ; Coarse sandy loam; Massive grade of structure; Earthy fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.1); Clear, Smooth change to - 
	A22	0.11 - 0.17 m	Dark yellowish brown (10YR4/4-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.12); Abrupt, Tongued change to
	B21	0.17 - 0.35 m	Yellowish brown (10YR5/6-Moist); Mechanical, 2.5Y42, 10-20% , 0-5mm, Prominent; 
	Mechanical, 10-20% ; Light clay; Strong grade of structure, 20-50 mm, Angular blocky; Strong 
	grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; , Calcareous, , ; , Gypseous, , 
	; Field pH 5.8 (Raupach, 0.3); Gradual change to - 
	B22	0.35 - 0.56 m	Yellowish brown (10YR5/8-Moist); ; Medium clay; Strong grade of structure, 50-100 mm, 
	Angular blocky; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); Gradual change to - 
	B3	0.56 - 0.66 m	Yellowish brown (10YR5/4-Moist); ; Light medium clay; Strong grade of structure, 50-100 mm, 
	Angular blocky; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); Gradual change to - 
	C	0.66 - 0.78 m	Light olive brown (2.5Y5/4-Moist); ; Coarse sandy medium clay; Moderate grade of structure, 
	50-100 mm, Prismatic; Moderate grade of structure, 20-50 mm, Angular blocky; Earthy fabric; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Kaylene Site 1
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T570	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	5.6C	0.13A	7.9B	1.9	0.71	0.11
	7A
	0.03 - 0.11	5.6C	0.1A	4.4B	0.97	0.3	0.08
	7.5A
	0.11 - 0.17	5.8C	0.07A
	7.6A
	0.17 - 0.35	6.2C	0.07A	7.8B	3.4	0.28	0.15
	7.3A
	0.35 - 0.56	6C	0.05A
	7.4A
	0.56 - 0.66	6.2C	0.05A
	7.5A
	0.66 - 0.78	6.3C	0.05A	6.8B	3.6	0.31	0.11
	7.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	2.1A	0.039A	0.12A	2.05A	45A	33	11	12
	0.03 - 0.11	0.94A	0.023A	0.04A	2.2A	44A	36	8	12
	0.11 - 0.17
	0.17 - 0.35	0.018A	1.47A
	0.35 - 0.56
	0.56 - 0.66	0.013A	1.23A
	0.66 - 0.78	0.24A	36A	31	9	24
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.11
	0.11 - 0.17
	0.17 - 0.35
	0.35 - 0.56
	0.56 - 0.66
	0.66 - 0.78

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T570	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method