Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T571	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	28/06/93	Elevation:	370 metres
	Map Ref.:	Sheet No. : 8159   GPS	Rainfall:	No Data
	Northing/Long.:	7847206 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	408867  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Schist 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Level
	Slope:	1 % 	Aspect:	280 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Thin Non-gravelly Silty 	Principal Profile Form:	Dr2.22
	Clayey Shallow
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	All necessary analytical data are available.	 soil
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - , , . *Species includes - Unknown species, Unknown species, Unknown species
	Mid Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.07 m	Dark reddish brown (2.5YR3/3-Moist); ; Silty clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.02); 
	Abrupt change to - 
	A2	0.07 - 0.22 m	Dark reddish brown (2.5YR3/4-Moist); ; Silty clay loam; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Dry; Rigid consistence; 90-100%, coarse gravelly, 20-60mm, 
	subangular tabular, dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Abrupt change to - 
	B2	0.22 - 0.44 m	Red (2.5YR4/8-Moist); ; Silty light clay; Strong grade of structure, 10-20 mm, Angular blocky; 
	Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Moderately moist; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); Gradual change to - 
	BC	0.44 - 0.55 m	Substrate influence, 10YR66, 10-20% , 0-5mm, Distinct; Substrate influence, 10-20% ; Silty light
	 clay; Strong grade of structure, 10-20 mm, Angular blocky; Strong grade of structure, 2-5 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T571	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	6.1C	0.11A	14B	3.7	1.4	0.09
	7.2A
	0.07 - 0.22	5.9C	0.08A
	7.3A
	0.22 - 0.44	5.6C	0.05A	20B	4.2	0.48	0.15
	7.3A
	0.44 - 0.55	6.2C	0.06A
	7.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	2A	0.105A	0.1A	0.82A	16A	39	19	26
	0.07 - 0.22
	0.22 - 0.44	0.057A	0.47A	14A	17	11	59
	0.44 - 0.55
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.22
	0.22 - 0.44
	0.44 - 0.55

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T571	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method