Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T574	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	20/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7841930 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	366823  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Kandosol Medium Non-gravelly 	Principal Profile Form:	Gn2.11
	Loamy Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa species, Dichanthium species, Aristida 
	species	Mid Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus similis
	Tall Strata - Tree, 12.01-20m, Isolated plants. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.03 m	Dark reddish brown (5YR3/2-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.02); 
	Clear change to - 
	A3	0.03 - 0.18 m	Dark reddish brown (2.5YR3/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.15); 
	Diffuse change to - 
	B1	0.18 - 0.47 m	Dusky red (10R3/4-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.4); Diffuse change 
	to - 
	B21	0.47 - 0.6 m	Dark red (10R3/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.55); 
	B22	0.6 - 0.8 m	Dark red (2.5YR3/6-Moist); ; Clay loam (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.7); 
	B22	0.8 - 1 m	Dark red (2.5YR3/6-Moist); ; Clay loam (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.9); 
	B22	1 - 1.2 m	Dark red (2.5YR3/6-Moist); ; Clay loam (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Kaylene Site 5
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T574	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	5.8C	0.08A	3.9B	1.5	0.53	0.06
	7A
	0.03 - 0.18	5.8C	0.04A
	7.1A
	0.18 - 0.47	5.7C	0.04A
	7.1A
	0.47 - 0.6	5.8C	0.03A	2.4B	0.74	0.47	0.04
	6.8A
	0.6 - 0.8	5.9C	0.03A
	6.8A
	0.8 - 1	6.2C	0.03A
	6.8A
	1 - 1.2	6.4C	0.02A	1.8E	1.2	0.32	0.09	5B	1.80
	6.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	0.95A	0.033A	0.05A	0.61A	42A	37	9	12
	0.03 - 0.18
	0.18 - 0.47
	0.47 - 0.6	0.24A	0.024A	0.6A	33A	30	6	31
	0.6 - 0.8
	0.8 - 1
	1 - 1.2	0.15A	35A	26	5	34
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.18
	0.18 - 0.47
	0.47 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T574	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method