Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T576	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	24/08/93	Elevation:	390 metres
	Map Ref.:	Sheet No. : 8058   GPS	Rainfall:	No Data
	Northing/Long.:	7804757 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	350846  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:	Active, Present (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Manganic Eutrophic Red Ferrosol Thin Non-gravelly Clay-	Principal Profile Form:	Gn3.11
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Dichanthium species, 
	Chrysopogon fallax	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus papuana, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	0-2%, medium gravelly, 6-20mm, rounded, Basalt
	Profile Morphology
	A1	0 - 0.01 m	Black (7.5YR2/0-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Subangular blocky; 
	Strong grade of structure, <2 mm, Angular blocky; Smooth-ped fabric; Dry; Very weak 
	consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.8 (Raupach, 0); 
	A3	0.01 - 0.1 m	Dark reddish brown (5YR3/2-Moist); ; Clay loam (Heavy); Strong grade of structure, 5-10 mm, 
	Angular blocky; Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Very weak consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.8 (Raupach, 0.07); 
	B1	0.1 - 0.19 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; 
	Very firm consistence; Common (10 - 20 %), Manganiferous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.6 (Raupach, 0.15); 
	B21	0.19 - 0.32 m	Dark reddish brown (5YR3/3-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; 
	Very firm consistence; Common (10 - 20 %), Manganiferous, Medium (2 -6 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	B22	0.32 - 0.47 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Subangular 
	blocky; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Very firm 
	consistence; Common (10 - 20 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ;
	 , Gypseous, , ; Field pH 6 (Raupach, 0.4); 
	0.47 - 0.65 m	Dark reddish brown (2.5YR3/4-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Very firm
	 consistence; Common (10 - 20 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , 
	; , Gypseous, , ; Field pH 6 (Raupach, 0.6); 

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T576	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	B23	0.65 - 0.9 m	Red (2.5YR4/6-Moist); Substrate influence, 7.5YR68, 2-10% , 0-5mm, Distinct; Substrate 
	influence, 2-10% ; Light medium clay; Strong grade of structure, 5-10 mm, Subangular blocky; 
	Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Very firm consistence; 
	Many (20 - 50 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6.8 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Kaylene Site 7
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T576	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.01	5.9C	0.08A	13B	5.4	1.6	5.4
	7A
	0.01 - 0.1	5.8C	0.07A	13B	5.5	1.6	0.08
	6.8A
	0.1 - 0.19	5.5C	0.05A
	7A
	0.19 - 0.32	5C	0.04A	8.6B	4.5	0.85	0.07
	6.5A
	0.32 - 0.47	5.3C	0.04A
	6.5A
	0.47 - 0.65	5.7C	0.03A
	6.6A
	0.65 - 0.9	5.9C	0.02A	6.9B	4.5	0.27	0.09
	6.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.01	2A	0.102A	0.41A	19A	17	27	37
	0.01 - 0.1	1.8A	0.098A	0.4A	18A	17	27	38
	0.1 - 0.19
	0.19 - 0.32	0.041A	0.34A	20A	10	15	56
	0.32 - 0.47
	0.47 - 0.65
	0.65 - 0.9	0.04A	0.19A	18A	7	9	66
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.01
	0.01 - 0.1
	0.1 - 0.19
	0.19 - 0.32
	0.32 - 0.47
	0.47 - 0.65
	0.65 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T576	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method