Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T579	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	19/08/93	Elevation:	590 metres
	Map Ref.:	Sheet No. : 7958   GPS	Rainfall:	No Data
	Northing/Long.:	7807176 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	314126  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Medium Slightly gravelly Clay-	Principal Profile Form:	Gn3.11
	loamy Clayey Shallow
	ASC Confidence:	Great Soil Group:	Euchrozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Dichanthium species, Themeda triandra
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus papuana
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus orgadophylla, Brachychiton 
	populneus
	Surface Coarse Fragments:	2-10%, stony, 200-600mm, subangular, Basalt
	Profile Morphology
	A1	0 - 0.02 m	Dark reddish brown (5YR3/3-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Platy; 
	Earthy fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0); 
	Clear change to - 
	AB	0.02 - 0.15 m	Dark reddish brown (5YR3/3-Moist); ; Light clay; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.1); 
	B21	0.15 - 0.26 m	Dark reddish brown (2.5YR3/4-Moist); ; Light medium clay; Moderate grade of structure, 20-50 
	mm, Subangular blocky; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; 
	Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); 
	B22	0.26 - 0.33 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Strong grade of structure, 5-10 mm, Polyhedral; 
	Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Very firm consistence; ,
	 Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Morphological Notes
	Observation Notes
	Kaylene Site 10
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T579	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.02	6.7A	0.11A	12B	3.9	1.7	0.07
	0.02 - 0.15	5.2C	0.07A
	6.5A
	0.15 - 0.26	5.3C	0.07A	9.1B	1.8	1	0.06
	6.5A
	0.26 - 0.33	5.3C	0.07A
	6.5A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.02	2.5A	0.233A	0.66A	6A	26	36	32
	0.02 - 0.15
	0.15 - 0.26	0.71A	0.213A	0.59A	2A	19	26	53
	0.26 - 0.33
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.02
	0.02 - 0.15
	0.15 - 0.26
	0.26 - 0.33

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T579	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method