Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T585	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	18/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7957   GPS	Rainfall:	No Data
	Northing/Long.:	7780576 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	338959  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Calcic Black Dermosol Medium Non-gravelly Silty Clayey	Principal Profile Form:	Dd2.43
	 Deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Unknown species, Unknown species, Unknown species
	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus platyphylla, Eucalyptus tessellaris
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus platyphylla, Eucalyptus tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Very dark grey (10YR3/1-Moist); ; Silty loam (Heavy); Moderate grade of structure, 2-5 mm, 
	Cast; Earthy fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.05); Clear change to - 
	A21e	0.08 - 0.16 m	Dark grey (10YR4/1-Moist); ; Silty loam (Heavy); Massive grade of structure; Earthy fabric; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.1); Clear change to
	 - 
	A3j	0.16 - 0.27 m	Dark grey (10YR4/1-Moist); ; Silty loam (Heavy); Weak grade of structure, 5-10 mm, Subangular
	 blocky; Earthy fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.2); Abrupt change to - 
	B21	0.27 - 0.56 m	Black (10YR2/1-Moist); ; Silty light clay; Strong grade of structure, 5-10 mm, Prismatic; Strong 
	grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Strong consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.5); Diffuse change to - 
	B22	0.56 - 0.82 m	Very dark grey (10YR3/1-Moist); ; Silty light clay; Moderate grade of structure, 5-10 mm, 
	Angular blocky; Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Very 
	strong consistence; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , 
	Gypseous, , ; Field pH 9.5 (Raupach, 0.8); Clear change to - 
	B23	0.82 - 1.16 m	Very dark grey (10YR3/1-Moist); ; Silty light clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Strong grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Very strong 
	consistence; Few (2 - 10 %), Calcareous, Fine (0 - 2 mm), Soft segregations; , Gypseous, , ; 
	Field pH 9.5 (Raupach, 1.1); Clear change to - 
	B3	1.16 - 1.32 m	Very dark grey (2.5Y3/1-Moist); ; Silty light clay; Strong grade of structure, 5-10 mm, Angular 
	blocky; Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Very strong 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 1.3); Clear change to - 
	1.32 - 1.61 m	Dark greyish brown (10YR4/2-Moist); ; Sandy clay loam (Heavy); Moderate grade of structure, 
	50-100 mm, Prismatic; Moderate grade of structure, 20-50 mm, Prismatic; Earthy fabric; Strong 
	consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 9 (Raupach, 1.5); 

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T585	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	1.61 - 1.92 m	Brown (10YR5/3-Moist); ; Fine sandy loam (Heavy); Moderate grade of structure, 50-100 mm, 
	Prismatic; Earthy fabric; Strong consistence; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 1.9); 
	Morphological Notes
	Observation Notes
	Kaylene Site 18
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T585	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.6C	0.2A	8.5E	7.3	0.74	2.6	32B	8.13
	6.8A
	0.08 - 0.16	5.3C	0.21A
	7.2A
	0.16 - 0.27	6.3C	0.31A
	7.7A
	0.27 - 0.56	7.9C	0.64A	9E	9.8	0.28	15	30B	50.00
	8.6A
	0.56 - 0.82	7.9C	0.7A
	8.8A
	0.82 - 1.16	7.9C	0.66A	7.2E	8.9	0.18	11	28B	39.29
	9.1A
	1.16 - 1.32	7.8C	0.41A
	8.9A
	1.32 - 1.61	7.2C	0.17A
	8.3A
	1.61 - 1.92	7C	0.1A	6.1E	6.1	0.05	1.7	15B	11.33
	8.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	2.3A	0.056A	0.14A	2.04A	3A	29	39	29
	0.08 - 0.16
	0.16 - 0.27
	0.27 - 0.56	0.57A	0.056A	0.03A	1.91A	2A	26	28	44
	0.56 - 0.82
	0.82 - 1.16	0.44A	0.05A	0.01A	1.94A	2A	31	27	39
	1.16 - 1.32
	1.32 - 1.61
	1.61 - 1.92	0.031A	2.51A	16A	58	9	17
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.16
	0.16 - 0.27
	0.27 - 0.56
	0.56 - 0.82
	0.82 - 1.16
	1.16 - 1.32
	1.32 - 1.61
	1.61 - 1.92

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	T585	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method