Project Name:
	Project Code:	DUSLARA	Site ID:	1436	Observation ID:	1
	Agency Name:	QLD Environment and Heritage
	Site Information
	Desc. By:	Lorimer, Mal	Locality:
	Date Desc.:	01/03/99	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	144.602638604015	Runoff:	Slow
	Easting/Lat.:	-21.4558756285602  Datum: GDA94	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Petroferric Red Sodosol     	Principal Profile Form:	Dr2.52
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	No effective disturbance. Natural
	Vegetation:
	Surface Coarse 
	Profile 
	A	0 - 0.07 m	; 
	B2t	0.07 - 0.64 m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	This is a very open  healthy system on shallow  red  sandy topsoil.

	Project Name:
	Project Code:	DUSLARA	Site ID:	1436	Observation 	1
	Agency Name:	QLD Environment and Heritage
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	4.7B	0.03A	1.16G	0.8	0.38	0.13	0.17G
	5.8A
	0.07 - 0.64	5.7B	0.03A	1.35G	2.34	0.1	0.35
	6.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	0.5A	2K	110B	2.4
	0.07 - 0.64	0.2A	2K	240B	15.48
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.07 - 0.64
	Laboratory Analyses Completed for this profile
	10D1	Potassium chloride - 40 sulfur (KCl-40)-S
	12A1_Cu	DTPA - extractable copper, zinc, manganese and iron
	12A1_Fe	DTPA - extractable copper, zinc, manganese and iron
	12A1_Mn	DTPA - extractable copper, zinc, manganese and iron
	12A1_Zn	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	14B1	Electrical conductivity/SE
	15D2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	automatic extractor
	15D2_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; mautomatic
	15D2_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; mautomatic
	15D2_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; mautomatic
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15K1	CEC - pH 8.2
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	18B1	Hydrochloric acid - extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	7B1	Water soluble nitrate - automated colour
	7D1a	Potentially mineralisable N, hot KCl extraction - automated colour, continuous segmented flow
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9C1	Olsen-extractable phosphorus - manual colour
	P10_GRAV	Gravel (%)
	P6_LP	Dispersion Index (Loveday and Pyle, 1973)