Project Name:
	Project Code:	DUSLARA	Site ID:	695	Observation ID:	1
	Agency Name:	QLD Environment and Heritage
	Site Information
	Desc. By:	Lorimer, Mal	Locality:
	Date Desc.:	01/03/99	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	145.884117426418	Runoff:	Slow
	Easting/Lat.:	-24.0835905336421  Datum: GDA94	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Alluvial plain
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Petroferric Red Chromosol     	Principal Profile Form:	Dr3.52
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site 	No effective disturbance. Natural
	Vegetation:
	Surface Coarse 
	Profile 
	A11	0 - 0.09 m	; 
	A12	0.09 - 0.65 m	; 
	B2t	0.65 - 1.35 m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	This is an open woodland of Corymbia dallachiana (ghost gum) and Corymbia species (bloodwood) with Acacia coriacea (desert oak) 
	understorey. Triodia species (spinifex) is the dominant ground layer species.

	Project Name:
	Project Code:	DUSLARA	Site ID:	695	Observation 	1
	Agency Name:	QLD Environment and Heritage
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.09	5.3B	0.02A	1.61G	0.53	0.23	0.06	0G
	6.4A
	0.09 - 0.65	5.8B	0.01A	1.1G	0.4	0.2	0.08	0G
	6.8A
	0.65 - 1.35	6.5B	0.02A	2.04G	1.65	0.45	0.08	0G
	7.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.09	1A	2K	83B	0.08
	0.09 - 0.65	0.1A	2K	52B	0.4
	0.65 - 1.35	0.1A	2K	89B	0.83
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.09
	0.09 - 0.65
	0.65 - 1.35
	Laboratory Analyses Completed for this profile
	10D1	Potassium chloride - 40 sulfur (KCl-40)-S
	12A1_Cu	DTPA - extractable copper, zinc, manganese and iron
	12A1_Fe	DTPA - extractable copper, zinc, manganese and iron
	12A1_Mn	DTPA - extractable copper, zinc, manganese and iron
	12A1_Zn	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	14B1	Electrical conductivity/SE
	15D2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; 
	automatic extractor
	15D2_K	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; mautomatic
	15D2_MG	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; mautomatic
	15D2_NA	Exchangeable bases and CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; mautomatic
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15K1	CEC - pH 8.2
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	18B1	Hydrochloric acid - extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	5A1	Chloride - 1:5 soil/water extract, potentiometric titration
	6A1	Organic carbon - Walkley and Black
	7B1	Water soluble nitrate - automated colour
	7D1a	Potentially mineralisable N, hot KCl extraction - automated colour, continuous segmented flow
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour

	9C1	Olsen-extractable phosphorus - manual colour
	P10_GRAV	Gravel (%)
	P6_LP	Dispersion Index (Loveday and Pyle, 1973)