Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	604	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Site Information
	Desc. By:	Locality:	Characterisation_Site: Morchard Hill (MORH). 
	Farmer_Contact: Mr Richard McCallum
	Date Desc.:	20/06/06	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	138.491	Runoff:	No Data
	Easting/Lat.:	-32.714	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.2 m	; 
	0.2 - 0.4 m	; 
	0.4 - 0.6 m	; 
	0.6 - 0.8 m	; 
	0.8 - 1 m	; 
	1 - 1.25 m	; 
	Morphological Notes
	Observation Notes
	Soil_Classification: Sandy Clay Loam over Light and Medium Clay. Soil_Comments: Moderate clay soil with moderate-high bulk 
	density, moderate-low CEC and a PAWC of 146mm. High EC below about 60cm and high chloride below about 90cm may limit 
	Site Notes
	Morchard

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	604	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.2	8.3A	0.3A	14.4E	2.4	1.2	0.3	18.3K	1.64
	0.2 - 0.4	8.6A	0.5A	11.2E	3.6	0.8	1	16.6K	6.02
	0.4 - 0.6	8.9A	1A	6.2E	4.7	0.5	1.9	13.2K	14.39
	0.6 - 0.8	8.8A	1.4A	4.4E	3.9	0.3	1.6	10.2K	15.69
	0.8 - 1	9.1A	1.1A	2.9E	3.8	0.3	1.3	8.3K	15.66
	1 - 1.25	8.9A	1.3A	3E	3.3	0.3	1.2	7.8K	15.38
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.2	1.17A	1.60	16	25
	0.2 - 0.4	0.74A	1.48	18	29
	0.4 - 0.6	0.43A	1.49	26	30
	0.6 - 0.8	0.26A	1.50	32	28
	0.8 - 1	0.15A	1.58	31	25
	1 - 1.25	0.17A	1.59	33	18
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.2
	0.2 - 0.4
	0.4 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.25

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	604	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15I3	CEC measurement - automated determination of ammonium and chloride ions
	15N1	Exchangeable sodium percentage (ESP)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_S	Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3A1	Bulk density - g/cm3
	P3B6VL_DUL	Drained Upper Limit (0.1 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_LL	Lower Limit (15 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_SAT	Saturated Moisture m3/m3 - Volumetric using APSRU in situ methodology