Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	697	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Site Information
	Desc. By:	Locality:	Characterisation_Site: Hill End. Farmer_Contact: Mr 
	Michael Pfitzner
	Date Desc.:	20/08/08	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	145.98584	Runoff:	No Data
	Easting/Lat.:	-34.02039	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.15 m	; 
	0.15 - 0.3 m	; 
	0.3 - 0.6 m	; 
	0.6 - 0.9 m	; 
	0.9 - 1.2 m	; 
	1.2 - 1.5 m	; 
	Morphological Notes
	Observation Notes
	Soil_Classification: Classification based on Particle size analysis. Sandy loam over a sandy clay loam. Soil_Comments: This soil 
	has a PAWC of 165mm for wheat to a depth of 180 cm. Soil data does not indicate any chemical constraints to cro
	Site Notes
	Griffith

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	697	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	6A	0.074A	5.29E	1.83	1.17	0.13
	0.15 - 0.3	7.1A	0.15A	12.94E	5.32	2.07	0.07
	0.3 - 0.6	8.1A	0.152A	8.83E	8.23	1.81	0.67
	0.6 - 0.9	8A	0.161A	10.31E	9.51	2.16	0.81
	0.9 - 1.2	8.1A	0.25A	5.84E	8.56	1.78	1.72
	1.2 - 1.5	8.3A	0.637A	2.31E	10.62	1.78	3.78
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	0.59A	1.68	4	20
	0.15 - 0.3	0.37A	1.52	7	34
	0.3 - 0.6	0.05A	1.42	14	21
	0.6 - 0.9	0.05A	1.52	16	21
	0.9 - 1.2	0.07A	1.56	19	24
	1.2 - 1.5	0.07A	1.46	18	34
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.6
	0.6 - 0.9
	0.9 - 1.2
	1.2 - 1.5

	Project Name:	APSRU Soil Reference Sites
	Project Code:	APSRU	Site ID:	697	Observation ID:	1
	Agency Name:	CSIRO Sustainable Ecosystems (QLD)
	Laboratory Analyses Completed for this profile
	12C2	Calcium chloride extractable boron - ICPAES
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15N1	Exchangeable sodium percentage (ESP)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	P10_HYD_C	Clay (%) - Hydrometer Method
	P10_HYD_S	Sand (%) - Hydrometer Method
	P10_HYD_Z	Silt (%) - Hydrometer Method
	P3A1	Bulk density - g/cm3
	P3B6VL_DUL	Drained Upper Limit (0.1 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_LL	Lower Limit (15 BAR) Moisture m3/m3 - Volumetric using APSRU in situ methodology
	P3B6VL_SAT	Saturated Moisture m3/m3 - Volumetric using APSRU in situ methodology