Project Name:	BAC
	Project Code:	BAC	Site ID:	T477	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:
	Date Desc.:	04/11/87	Elevation:	<20 metres
	Map Ref.:	Sheet No. : 8063   1:100000	Rainfall:	0
	Northing/Long.:	145.944444444444	Runoff:	No runoff
	Easting/Lat.:	-17.3583333333333	Drainage:	Very poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Swamp	Slope Category:	No Data
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Regolithic Acidic Fibric Organosol     	Principal Profile Form:	O
	ASC Confidence:	Great Soil Group:	Acid peat
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Black (10YR2/1-Moist); ; Loam (Sapric); Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Moist; Very weak consistence; Common, fine (1-2mm) roots; 
	A1	0.15 - 0.3 m	Black (10YR2/1-Moist); ; Loam (Sapric); Moderate grade of structure, 5-10 mm, Subangular 
	blocky; Moist; Very weak consistence; Few, fine (1-2mm) roots; 
	A3	0.3 - 0.45 m	Very dark grey (10YR3/1-Moist); ; Loam (Sapric); Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Wet; Very weak consistence; Few, fine (1-2mm) roots; 
	0.45 - 0.7 m	Very dark grey (10YR3/1-Moist); ; 
	0.7 - 1 m	Very dark grey (10YR3/1-Moist); ; 
	1 - 1.4 m	Very dark greyish brown (10YR3/2-Moist); ; 
	1.4 - 1.7 m	Dark greyish brown (10YR4/2-Moist); ; 
	1.7 - 2.05 m	Dark brown (7.5YR3/2-Moist); ; 
	2.05 - 2.15 m	Greyish brown (2.5Y5/2-Moist); ; 
	Morphological Notes
	Observation Notes
	CLEARED REGROWTH OF ME QUI PANDANUS & FLINDERSIA & RF Spp. 130-133 10YR53? CLAYEY LAYER.                              
	  
	Site Notes
	BABINDA SWAMP

	Project Name:	BAC
	Project Code:	BAC	Site ID:	T477	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	4.32A	 0.089A	 0.36H	 0.27	 0.09	 0.16	 7.87F	 9.24A	 8.8F	1.73
	 80C	0.20
	0.15 - 0.3	4.45A	 0.053A	 0.4H	 0.13	 0.09	 0.11	 7.42F	 8.76A	 8.2F	1.26
	 79C	0.14
	0.3 - 0.45	4.65A	 0.05A	 0.36H	 0.2	 0.05	 0.12	 8.54F	 9.49A	 9.3F	1.26
	 66C	0.18
	0.45 - 0.7	4.23A	 0.115A	 1.17H	 1.23	 0.06	 0.36	 11.4F	 5.03A	 14.2F	7.16
	 102C	0.35
	0.7 - 1	4.21A	 0.087A	 0.43H	 1.73	 0.05	 0.38	 12.1F	 11A	 14.7F	3.45
	1 - 1.4	4.68A	 0.041A	 0.34H	 1.18	 0.1	 0.34	 9.18F	 9.42A	 11.1F	3.61
	 53C	0.64
	1.4 - 1.7	4.81A	 0.038A	 0.3H	 1.09	 0.16	 0.27	 7.29F	 7.66A	 9.1F	3.52
	 39C	0.69
	1.7 - 2.05	5.03A	 0.016A	 0.18H	 1.73	 0.25	 0.43	 9.11F	 14.7A	 11.7F	2.93
	 74C	0.58
	2.05 - 2.15	4.9A	 0.04A	 0.07H	 0.95	 0.23	 0.15	 5.25F	 7.31A	 6.7F	2.05
	 16C	0.94
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 29.5C	 84A	 2A
	 20B
	0.15 - 0.3	 31.2C	 3A	 1.6A
	 13B
	0.3 - 0.45	 35.3C	 0.88A
	0.45 - 0.7	 40.3C	 0.83A
	0.7 - 1	 47.9C	<2A	 0.92A
	 7B
	1 - 1.4	 33C	 0.61A
	1.4 - 1.7	 21.9C	 0.34A
	1.7 - 2.05	 25.1C	 5A	 0.51A
	 23B
	2.05 - 2.15	 4.1C	 8A	 0.1A
	 26B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.3 - 0.45
	0.45 - 0.7
	0.7 - 1
	1 - 1.4
	1.4 - 1.7
	1.7 - 2.05
	2.05 - 2.15

	Project Name:	BAC
	Project Code:	BAC	Site ID:	T477	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)