Project Name:	BAC
	Project Code:	BAC	Site ID:	T480	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	In magazine reserve.
	Date Desc.:	08/12/87	Elevation:	<20 metres
	Map Ref.:	Sheet No. : 8063   1:100000	Rainfall:	0
	Northing/Long.:	145.748888888889	Runoff:	Slow
	Easting/Lat.:	-17.0002777777778	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Alluvial fan
	3%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Very gently sloped
	Slope:	0.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Magnesic Yellow Dermosol     	Principal Profile Form:	Gn3.04
	ASC Confidence:	Great Soil Group:	Yellow podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:
	Tall Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Melaleuca viridiflora, Acacia species, Trigonella suavissima
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.17 m	Greyish brown (10YR5/2-Moist); ; Fine sandy loam (Heavy); Moderate grade of structure, 2-5 
	mm, Cast; Moist; Weak consistence; Few, fine (1-2mm) roots; Gradual change to - 
	A1	0.14 - 0.27 m	Greyish brown (10YR5/2-Moist); , 10YR63, 10-20% , 5-15mm, Faint; , 10-20% , 5-15mm, Faint; 
	Fine sandy loam (Heavy); Moderate grade of structure, 2-5 mm, Cast; Moderately moist; Weak 
	consistence; Few, fine (1-2mm) roots; Gradual change to - 
	A2	0.27 - 0.49 m	Very pale brown (10YR7/3-Moist); ; Silty clay loam; Massive grade of structure; Moderately 
	moist; Weak consistence; Few, fine (1-2mm) roots; Clear change to - 
	B21	0.49 - 0.56 m	Light yellowish brown (10YR6/4-Moist); , 2.5Y70, 20-50% , 15-30mm, Distinct; , 5YR48, 20-
	50% , 15-30mm, Distinct; Medium clay; Moderate grade of structure, 20-50 mm, Angular blocky; 
	Smooth-ped fabric; Moderately moist; Strong consistence; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; 
	B21	0.56 - 0.82 m	Light yellowish brown (10YR6/4-Moist); , 2.5Y70, 20-50% , 15-30mm, Distinct; , 5YR48, 20-
	50% , 15-30mm, Distinct; Heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; 
	Smooth-ped fabric; Dry; Strong consistence; Few (2 - 10 %), Ferromanganiferous, Very 
	coarse (20 - 60 mm), Nodules; Diffuse change to - 
	B22	0.82 - 1.13 m	Brownish yellow (10YR6/6-Moist); , 2.5Y70, 20-50% , 15-30mm, Distinct; , 2.5YR46, 20-50% , 
	15-30mm, Distinct; Heavy clay; Strong grade of structure, 20-50 mm, Angular blocky; Smooth-
	ped fabric; Dry; Strong consistence; Few (2 - 10 %), Ferromanganiferous, Coarse (6 - 20 mm), 
	Nodules; Diffuse change to - 
	B3	1.13 - 1.48 m	Light grey (2.5Y7/0-Moist); , 10YR56, 20-50% , 30-mm, Prominent; , 5YR46, 20-50% , 30-mm, 
	Prominent; Sandy light clay; Weak grade of structure, 50-100 mm, Angular blocky; Dry; Strong 
	consistence; 
	B3	1.48 - 1.83 m	Light grey (2.5Y7/0-Moist); , 10YR56, 20-50% , 30-mm, Prominent; , 5YR46, 20-50% , 30-mm, 
	Prominent; Sandy light clay; Weak grade of structure, 50-100 mm, Angular blocky; Dry; Strong 
	consistence; Diffuse change to - 

	Project Name:	BAC
	Project Code:	BAC	Site ID:	T480	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	1.83 - 2.02 m	Yellowish red (5YR4/6-Moist); , 10YR66, 20-50% , 30-mm, Faint; , 10YR71, 20-50% , 30-mm, 
	Faint; Sandy clay loam; Massive grade of structure; Dry; Very firm consistence; 10-20%, fine 
	gravelly, 2-6mm, subangular, Quartz, coarse fragments; 
	Morphological Notes
	Observation Notes
	VEGETATION IS ALL REGROWTH: 14-49CM VERY DILATENT.                                                                      
	Site Notes
	QUEERAH

	Project Name:	BAC
	Project Code:	BAC	Site ID:	T480	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.14	5.15A	 0.048A	 0.89H	 0.54	 0.08	 0.04	 1.1F	 2A	 2.7F	2.00
	 3.7C	1.08
	0.14 - 0.27	5.46A	 0.023A
	0.27 - 0.49	5.25A	 0.015A	 0.1H	 0.1	 0.02	<0.02	 1.05F	 1.1A	 1.3F
	 1.7C
	0.49 - 0.56	5.86A	 0.008A	<0.02H	 0.6	 0.02	<0.02	 1.33F	 1.4A	 2F
	 2.5C
	0.56 - 0.82	5.82A	 0.009A	 0.07H	 0.78	 0.94	<0.02	 2.16F	 2.9A	 4F
	 3.5C
	0.82 - 1.13	5.76A	 0.012A
	1.13 - 1.48	5.8A	 0.008A	 0.09H	 0.92	 0.02	<0.02	 2.4F	 3A	 3.5F
	 3.9C
	1.48 - 1.83	5.44A	 0.009A
	1.83 - 2.02	5.34A	 0.008A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.14	 1.71C	 4B	 0.02A	 0.06A	 0.56A	 1	 5A	 54	 28	 13
	0.14 - 0.27	 0.83C	<2B	 0.03A	 1	 5A	 48	 33	 14
	0.27 - 0.49	 0.33C	<2B	 0.01A	 0.02A	 0.59A	 3	 5A	 51	 29	 15
	0.49 - 0.56	 0.15C	<2B	 27	 7A	 41	 27	 25
	0.56 - 0.82	<2B	 11	 8A	 31	 29	 35
	0.82 - 1.13	 18	 6A	 31	 27	 35
	1.13 - 1.48	 1	 11A	 37	 24	 38
	1.48 - 1.83	 8	 18A	 36	 21	 24
	1.83 - 2.02	 0	 48A	 19	 14	 19
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.14
	0.14 - 0.27
	0.27 - 0.49
	0.49 - 0.56
	0.56 - 0.82
	0.82 - 1.13
	1.13 - 1.48
	1.48 - 1.83
	1.83 - 2.02

	Project Name:	BAC
	Project Code:	BAC	Site ID:	T480	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)