Project Name:	BAC
	Project Code:	BAC	Site ID:	T486	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.G. Murtha	Locality:	3m south of drain in corner of virgin forest.
	Date Desc.:	09/12/87	Elevation:	<20 metres
	Map Ref.:	Sheet No. : 8063   1:100000	Rainfall:	0
	Northing/Long.:	145.929444444444	Runoff:	No runoff
	Easting/Lat.:	-17.2038888888889	Drainage:	Very poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Closed Depression	Relief:	No Data
	Elem. Type:	Swamp	Slope Category:	Level
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Dermosolic Redoxic Hydrosol     	Principal Profile Form:	Uf6.33
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, 20.01-35m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.17 m	Dark greyish brown (10YR4/2-Moist); ; Silty medium clay; Moderate grade of structure, 5-10 
	mm, Cast; Moist; Weak consistence; Common, fine (1-2mm) roots; Clear change to - 
	B21	0.17 - 0.32 m	Greyish brown (2.5Y5/2-Moist); , 5YR46, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; 
	Silty medium clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped 
	fabric; Moist; Weak consistence; Common, very fine (0-1mm) roots; 
	B21	0.32 - 0.45 m	Greyish brown (2.5Y5/2-Moist); , 7.5YR56, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; 
	Silty medium clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped 
	fabric; Moist; Firm consistence; Few, very fine (0-1mm) roots; Diffuse change to - 
	B22	0.45 - 0.68 m	Greyish brown (2.5Y5/2-Moist); , 7.5YR56, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; 
	Silty medium clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped 
	fabric; Moist; Firm consistence; Few, very fine (0-1mm) roots; Clear change to - 
	2A1	0.68 - 0.76 m	Dark grey (10YR4/1-Moist); , 2.5Y52, 10-20% , 5-15mm, Distinct; , 10YR44, 10-20% , 5-15mm, 
	Distinct; Silty light clay; Weak grade of structure, 20-50 mm, Subangular blocky; Smooth-ped 
	fabric; Wet; Firm consistence; Few, very fine (0-1mm) roots; Clear change to - 
	2B2	0.76 - 1.01 m	Grey (5Y5/1-Moist); , 10YR46, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; Silty medium 
	clay; Weak grade of structure, 20-50 mm, Subangular blocky; Smooth-ped fabric; Wet; Firm 
	consistence; Few, very fine (0-1mm) roots; Gradual change to - 
	D	1.01 - 1.12 m	Brown (10YR5/3-Moist); , 10YR22, 10-20% , 5-15mm, Distinct; , 10-20% , 5-15mm, Distinct; 
	Clayey peat; Massive grade of structure; Wet; Very weak consistence; Gradual change to - 
	D	1.12 - 1.38 m	Very dark brown (10YR2/2-Moist); ; Fibric peat; Massive grade of structure; Wet; Very weak 
	consistence; Diffuse change to - 
	D	1.38 - 1.6 m	Very dark brown (10YR2/2-Moist); ; Fibric peat; Massive grade of structure; Wet; Very weak 
	consistence; 
	D	1.6 - 1.88 m	Black (10YR2/1-Moist); ; Fibric peat; Massive grade of structure; Wet; Very weak consistence; 
	Morphological Notes
	Observation Notes
	VEGETATION IS MIXTURE OF MEQUI PALMS AND  RAINFOREST SPECIES.                                                           

	Project Name:	BAC
	Project Code:	BAC	Site ID:	T486	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	DERALL EAST

	Project Name:	BAC
	Project Code:	BAC	Site ID:	T486	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.17	4.47A	 0.185A	 1.49H	 1.23	 0.18	 0.05	 2.82F	 5.2A	 5.8F	0.96
	 15.1C	0.33
	0.17 - 0.32	4.82A	 0.08A	 1.07H	 0.75	 0.07	 0.18	 3.2F	 3.9A	 5.3F	4.62
	 9.6C	1.88
	0.32 - 0.45	5.07A	 0.056A	 0.87H	 0.78	 0.04	 0.22	 2.66F	 3.4A	 4.6F	6.47
	0.45 - 0.68	5.03A	 0.118A	 0.16H	 0.16	 0.05	 0.03	 2.76F	 1.8A	 3.2F	1.67
	 10.4C	0.29
	0.68 - 0.76	4.91A	 0.162A	 0.54H	 0.75	 0.02	 0.16	 2.52F	 2A	 4F	8.00
	0.76 - 1.01	4.96A	 0.124A	 0.48H	 0.91	 0.04	 0.13	 2.95F	 2.3A	 4.5F	5.65
	1.01 - 1.12	4.67A	 0.19A	 0.51H	 0.6	 0.02	 0.04	 2.26F	 3.7A	 3.4F	1.08
	1.12 - 1.38	2.87A	 3.13A	 0.67H	 0.61	<0.02	 0.04	 36.6F	 5.9A	 37.9F	0.68
	1.38 - 1.6
	1.6 - 1.88
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.17	 4.44C	 46B	 0.12A	 0.15A	 2.6A	 0	 3A	 5	 61	 30
	0.17 - 0.32	 1.9C	 54B	 0.09A	 0.1A	 2.75A	 0	 1A	 4	 62	 34
	0.32 - 0.45	 1.6C	 102B	 0.08A	 0	 1A	 5	 62	 32
	0.45 - 0.68	 168B	 0.11A	 2.73A	 0	 1A	 6	 54	 39
	0.68 - 0.76	 2.09C	 0.07A	 0	 1A	 5	 57	 36
	0.76 - 1.01	 2.02C	 0.06A	 0	 0A	 4	 48	 48
	1.01 - 1.12	 0	 2A	 17	 48	 34
	1.12 - 1.38	 7B	 0.03A	 1.87A	 0	 19A	 15	 49	 17
	1.38 - 1.6
	1.6 - 1.88
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.17
	0.17 - 0.32
	0.32 - 0.45
	0.45 - 0.68
	0.68 - 0.76
	0.76 - 1.01
	1.01 - 1.12
	1.12 - 1.38
	1.38 - 1.6
	1.6 - 1.88

	Project Name:	BAC
	Project Code:	BAC	Site ID:	T486	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	13C1_FE	Citrate/dithionite-extractable iron, aluminium, Manganese and Silicon
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15D1_CEC	CEC - 1M ammonium acetate at pH 7.0, pretreatment for soluble salts; manual leach
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6B3	Total organic carbon - high frequency induction furnace, infrared
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	9H1	Phosphate retention
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)