Project Name:	BL
	Project Code:	BL	Site ID:	B298	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	22/10/56	Elevation:	No Data
	Map Ref.:	Sheet No. : 8850   1:100000	Rainfall:	635
	Northing/Long.:	148.81944	Runoff:	Moderately rapid
	Easting/Lat.:	-23.575	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Cz	Substrate Material:	Auger boring, 1.9 m deep,Porous, Mudstone 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Self-Mulching Black Vertosol  	Principal Profile Form:	Ug5.15
	   
	ASC Confidence:	Great Soil Group:	Brown clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Chloris species
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Acacia harpophylla, Atalaya hemiglauca, Eremophila mitchellii
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, , Quartz
	Profile Morphology
	AB	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Heavy clay; Strong grade of structure, 2-5 mm, 
	Granular; Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Very 
	few (0 - 2 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 8.7 (pH meter); Gradual change
	B2	0.3 - 0.61 m	Very dark greyish brown (10YR3/2-Moist); ; Heavy clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments;
	 Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; Field pH 8.9 (pH meter); Gradual 
	change to - 
	B2	0.76 - 1.07 m	Reddish brown (5YR4/4-Moist); ; Heavy clay; Moderate grade of structure, Lenticular; Moist; 
	Firm consistence; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; Field pH 8.4 (pH 
	meter); Gradual change to - 
	B2	1.07 - 1.37 m	Yellowish red (5YR4/6-Moist); ; Heavy clay; Moderate grade of structure, Lenticular; Moist; Firm
	 consistence; Field pH 5.5 (pH meter); Diffuse change to - 
	B2	1.37 - 1.57 m	Yellowish red (5YR4/6-Moist); , 7.5YR56; Heavy clay; Moderate grade of structure, Lenticular; 
	Moist; Firm consistence; Field pH 5 (pH meter); Diffuse change to - 
	B3	1.68 - 1.9 m	Strong brown (7.5YR5/6-Moist); ; Medium clay; Weak grade of structure, Lenticular; Moist; 
	Weak consistence; 0-2%, Mudstone, coarse fragments; Field pH 4.8 (pH meter); Diffuse change
	C	1.98 - 2.08 m	Strong brown (7.5YR5/6-Moist); ; Light clay; Massive grade of structure; Moist; Weak 
	consistence; 2-10%, coarse gravelly, 20-60mm, Mudstone, coarse fragments; Field pH 4.4 (pH 
	meter); 
	Morphological Notes
	Observation Notes
	0-10CM GRANULAR GRADING TO BLOCKY STRUCTURE: ALKALINE OVER ACID CLAYS                                                   
	Site Notes
	BLACKWATER

	Project Name:	BL
	Project Code:	BL	Site ID:	B298	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8.7H	 0.05B	 31.7K	 9.4	 0.73	 0.71
	0.3 - 0.61	8.9H	 0.42B
	0.76 - 1.07	8.4H	 0.7B	 16.1K	 17.6	 0.28	 8.2
	1.07 - 1.37	5.5H	 0.6B
	1.37 - 1.57	5H	 0.58B	 7D
	1.68 - 1.9	4.8H	 0.55B
	1.98 - 2.08	4.4H	 0.54B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 2.22C	 1.06A	 16C	 0.069F	 0.12B	1.30	 0.3	 5C	 28	 14	 47
	0.3 - 0.61	 4.37C	 0.68A	 0.07B	1.30	 1	 3C	 23	 19	 47
	0.76 - 1.07	 0.67C	 0.03B	1.30	 3C	 20	 17	 59
	1.07 - 1.37	 0.04B	1.30
	1.37 - 1.57	 1C	 22	 25	 55
	1.68 - 1.9
	1.98 - 2.08	 0.066F	 1C	 32	 24	 44
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1	 0.44C	 0.25C
	0.3 - 0.61	 0.45C	 0.27C
	0.76 - 1.07	 0.49C	 0.27C
	1.07 - 1.37	 0.5C	 0.26C
	1.37 - 1.57
	1.68 - 1.9
	1.98 - 2.08

	Project Name:	BL
	Project Code:	BL	Site ID:	B298	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate