Project Name:	BL
	Project Code:	BL	Site ID:	B317	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	12/07/57	Elevation:	No Data
	Map Ref.:	Sheet No. : 8944   1:100000	Rainfall:	660
	Northing/Long.:	150.463888888889	Runoff:	Moderately rapid
	Easting/Lat.:	-26.55	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Existing vertical exposure	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	   T	Substrate Material:	Existing vertical exposure, 0.99 m deep,No 
	Data
	Land Form
	Rel/Slope Class: 	Rolling plains <9m 10-32%	Pattern Type:	Peneplain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Kandosol     	Principal Profile Form:	Gn2.22
	ASC Confidence:	Great Soil Group:	Yellow earth
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Aristida species
	Mid Strata - Tree, 3.01-6m, Closed or dense. *Species includes - Acacia species
	Tall Strata - Tree, 6.01-12m, Closed or dense. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Reddish brown (5YR4/4-Moist); ; Clay loam; Moderate grade of structure, 10-20 mm, Polyhedral;
	 Moist; Very weak consistence; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Nodules; Field 
	pH 5.4 (pH meter); Many, very fine (0-1mm) roots; Gradual change to - 
	B11	0.1 - 0.28 m	Yellowish red (5YR5/6-Moist); ; Light clay; Weak grade of structure, 10-20 mm, Polyhedral; 
	Moist; Weak consistence; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Nodules; Field pH 5.6
	 (pH meter); Common, very fine (0-1mm) roots; Gradual change to - 
	B12	0.28 - 0.51 m	Yellowish brown (10YR5/6-Moist); ; Light medium clay; Massive grade of structure; Moist; 
	Weak consistence; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Nodules; Field pH 6.4 (pH 
	meter); Common, very fine (0-1mm) roots; Gradual change to - 
	B21	0.51 - 0.74 m	Yellowish brown (10YR5/4-Moist); ; Medium clay; Massive grade of structure; Dry; Very firm 
	consistence; Few (2 - 10 %), Ferruginous, , Nodules; Field pH 7.3 (pH meter); Few, very fine 
	(0-1mm) roots; Gradual change to - 
	B22	0.74 - 0.86 m	Yellowish brown (10YR5/8-Dry); , 10YR71, 20-50% , 5-15mm, Distinct; , 10YR62, 20-50% , 5-
	15mm, Distinct; Heavy clay; Weak grade of structure, 10-20 mm, Polyhedral; Dry; Very firm 
	consistence; Few (2 - 10 %), , , Nodules; Field pH 7.7 (pH meter); Gradual change to - 
	B3	0.86 - 0.97 m	Yellowish brown (10YR5/6-Moist); , 10YR61, 20-50% , 5-15mm, Prominent; , 20-50% , 5-15mm,
	 Prominent; Heavy clay; Weak grade of structure, Lenticular; Dry; Very firm consistence; Very 
	few (0 - 2 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 7.8 (pH meter); Gradual 
	change to - 
	C	0.99 - 1.07 m	Red (2.5YR4/6-Dry); , 10YR81, 20-50% , 15-30mm, Prominent; , 20-50% , 15-30mm, Prominent; 
	Massive grade of structure; Dry; , Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 8 (pH 
	meter); 
	C	1.07 - 1.17 m	; 
	Morphological Notes
	C	Hard indurated rock-like mottled zone:
	Observation Notes

	Project Name:	BL
	Project Code:	BL	Site ID:	B317	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	CHINCHILLA

	Project Name:	BL
	Project Code:	BL	Site ID:	B317	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.4H	 0.01C	 2.8K	 2.3	 0.12	 0.15	 13.4J	1.12
	0.1 - 0.28	5.6H	 0.01C
	0.28 - 0.51	6.4H	 0.01C	 1.1K	 2.8	 0.02	 0.61	 8J	7.63
	0.51 - 0.74	7.3H	 0.02C
	0.74 - 0.86	7.7H	 0.04C	 1.6K	 6.3	 0.02	 2.8	 13J	21.54
	0.86 - 0.97	7.8H	 0.05C
	0.99 - 1.07	8H	 0.05C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 1.17E	 2C	 0.006F	 0.1B	 2	 13C	 44	 14	 27
	0.1 - 0.28	 0.34E	 6	 13C	 41	 11	 36
	0.28 - 0.51	 0.15E	 8	 15C	 37	 9	 40
	0.51 - 0.74	 4	 13C	 33	 9	 47
	0.74 - 0.86	 3	 10C	 28	 8	 55
	0.86 - 0.97	 0.04C	 2	 13C	 32	 6	 49
	0.99 - 1.07
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.1 - 0.28
	0.28 - 0.51
	0.51 - 0.74
	0.74 - 0.86
	0.86 - 0.97
	0.99 - 1.07

	Project Name:	BL
	Project Code:	BL	Site ID:	B317	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded