Project Name:	BL
	Project Code:	BL	Site ID:	B326	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	14/10/57	Elevation:	 293 metres
	Map Ref.:	Sheet No. : 8942   1:100000	Rainfall:	0
	Northing/Long.:	150.033333333333	Runoff:	Very slow
	Easting/Lat.:	-27.5305555555556	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	 Klg	Substrate Material:	Auger boring, 2 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	18 metres
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Epipedal Grey Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Brown clay
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Chloris species
	Mid Strata - Tree, 3.01-6m, Closed or dense. *Species includes - Eremophila mitchellii, Geijera parviflora
	Tall Strata - Tree, 6.01-12m, Closed or dense. *Species includes - Casuarina cristata, Acacia harpophylla
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	AB	0 - 0.15 m	Dark greyish brown (10YR4/2-Dry); ; Heavy clay; Strong grade of structure, 2-5 mm, Granular; 
	Dry; Loose consistence; Field pH 7.5 (pH meter); Gradual change to - 
	B2	0.15 - 0.41 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Moist; Firm consistence; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Soft 
	segregations; Field pH 8.5 (pH meter); Gradual change to - 
	B2	0.46 - 0.76 m	Dark greyish brown (10YR4/2-Moist); ; Heavy clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Moist; Firm consistence; Field pH 5.3 (pH meter); Gradual change to - 
	B2	0.76 - 1.22 m	Brown (7.5YR4/2-Moist); ; Heavy clay; Moderate grade of structure, Angular blocky; Moist; Firm
	 consistence; Field pH 4.3 (pH meter); Gradual change to - 
	B2	1.22 - 1.75 m	Brown (7.5YR4/2-Moist); ; Heavy clay; Moderate grade of structure, Lenticular; Moist; Firm 
	consistence; Field pH 4.2 (pH meter); Gradual change to - 
	B2	1.75 - 2.29 m	Brown (7.5YR4/2-Moist); ; Heavy clay; Moderate grade of structure, Lenticular; Moist; Firm 
	consistence; Field pH 4.3 (pH meter); 
	B3	2.29 - 2.84 m	; Medium clay; Moist; 
	B3	2.9 - 3.35 m	; Light clay; Moist; 
	B3	3.96 - 4.27 m	; Clay loam; Moist; 
	B3	4.42 - 5.79 m	; Heavy clay; Moist; 
	C	5.79 - 6.1 m	; Heavy clay; 
	C	6.4 - 6.71 m	; Heavy clay; 
	Morphological Notes
	Observation Notes
	BANK PROFILE: 0-15CM GRANULAR GRADING TO BLOCKY STRUCTURE:                                                              

	Project Name:	BL
	Project Code:	BL	Site ID:	B326	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	TARA

	Project Name:	BL
	Project Code:	BL	Site ID:	B326	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	7.5H	 0.07C
	0.15 - 0.41	8.5H	 0.15C
	0.46 - 0.76	5.3H	 0.48C
	0.76 - 1.22	4.3H	 0.77C
	1.22 - 1.75	4.2H	 0.69C
	1.75 - 2.29	4.3H	 0.64C	 3.8K	 13.6	 0.32	 7.8	 38J	20.53
	2.29 - 2.84	4.4H	 0.51C
	2.9 - 3.35	4.5H	 0.43C
	3.96 - 4.27	4.6H	 0.46C
	4.42 - 5.79	4.5H	 0.55C
	5.79 - 6.1	4.6H	 0.68C
	6.4 - 6.71	5H	 0.79C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 1.72E	 17C	 0.04F	 2C	 23	 13	 57
	0.15 - 0.41
	0.46 - 0.76	 0.47E	 0.026F	 2C	 20	 13	 62
	0.76 - 1.22
	1.22 - 1.75
	1.75 - 2.29	 0.031F	 1C	 13	 17	 68
	2.29 - 2.84
	2.9 - 3.35	 0.03F	 3C	 38	 26	 33
	3.96 - 4.27
	4.42 - 5.79	 0.036F	 2C	 17	 23	 60
	5.79 - 6.1	 0.022F	 2C	 7	 30	 64
	6.4 - 6.71
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.41
	0.46 - 0.76
	0.76 - 1.22
	1.22 - 1.75
	1.75 - 2.29
	2.29 - 2.84
	2.9 - 3.35
	3.96 - 4.27
	4.42 - 5.79
	5.79 - 6.1
	6.4 - 6.71

	Project Name:	BL
	Project Code:	BL	Site ID:	B326	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	MIN_EC	Exchange Capacity - Minerology
	MIN_NR_K2O	Kaolin minerals
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mi	Mica - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction