Project Name:	BL
	Project Code:	BL	Site ID:	B332	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	01/10/57	Elevation:	 229 metres
	Map Ref.:	Sheet No. : 8841   1:100000	Rainfall:	0
	Northing/Long.:	149.716666666667	Runoff:	Slow
	Easting/Lat.:	-28	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qs	Substrate Material:	Auger boring, 3 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Endoacidic Epipedal Grey Vertosol     	Principal Profile Form:	Ug5.24
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Chloris species
	Mid Strata - Tree, 3.01-6m, Closed or dense. *Species includes - Acacia harpophylla
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	AB	0 - 0.07 m	Greyish brown (10YR5/2-Dry); ; Light medium clay; Strong grade of structure, Granular; Dry; 
	Firm consistence; Field pH 6.3 (pH meter); Many, very fine (0-1mm) roots; Clear change to - 
	B2	0.07 - 0.23 m	Dark greyish brown (10YR4/2-Dry); , 10YR62, 20-50% , 0-5mm, Faint; , 7.5YR54, 20-50% , 0-
	5mm, Faint; Heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; Dry; Strong 
	consistence; , Manganiferous, Fine (0 - 2 mm), Soft segregations; Field pH 6.7 (pH meter); 
	Common, very fine (0-1mm) roots; Gradual change to - 
	B2	0.23 - 0.46 m	Dark greyish brown (10YR4/2-Dry); , 5YR54, 20-50% , 0-5mm, Faint; , 10YR62, 20-50% , 0-
	5mm, Faint; Heavy clay; Moderate grade of structure, Angular blocky; Dry; Strong consistence; 
	Field pH 4.9 (pH meter); Gradual change to - 
	B2	0.46 - 0.91 m	Reddish brown (5YR5/4-Moist); , 7.5YR42, 20-50% , 0-5mm, Faint; , 10YR62, 20-50% , 0-5mm, 
	Faint; Heavy clay; Moderate grade of structure, Lenticular; Moderately moist; Strong 
	consistence; Field pH 4.4 (pH meter); Diffuse change to - 
	B2	0.91 - 1.6 m	Reddish brown (5YR5/4-Moist); , 10YR71, 20-50% , 0-5mm, Faint; , 2.5YR36, 20-50% , 0-5mm, 
	Faint; Heavy clay; Moderate grade of structure, Lenticular; Moderately moist; Strong 
	consistence; Field pH 4.3 (pH meter); Diffuse change to - 
	B3	1.6 - 2.08 m	Reddish yellow (5YR6/6-Moist); , 10YR71, 20-50% , 0-5mm, Faint; , 20-50% , 0-5mm, Faint; 
	Medium clay; Weak grade of structure, Angular blocky; Moderately moist; Strong consistence; 
	Field pH 4.3 (pH meter); Diffuse change to - 
	B3	2.08 - 2.49 m	Reddish yellow (5YR6/6-Moist); , 10YR71, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, 
	Distinct; Light clay; Weak grade of structure, Angular blocky; Dry; Strong consistence; Field pH 
	4.3 (pH meter); Diffuse change to - 
	B3	2.49 - 3 m	Reddish yellow (5YR6/6-Moist); , 10YR71, 20-50% , 5-15mm, Distinct; , 20-50% , 5-15mm, 
	Distinct; Light medium clay; Weak grade of structure, Angular blocky; Moderately moist; Very 
	firm consistence; Field pH 4.1 (pH meter); Diffuse change to - 

	Project Name:	BL
	Project Code:	BL	Site ID:	B332	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	D	3.05 - 3.66 m	Red (10R4/6-Moist); , 2.5Y62, 20-50% , 15-30mm, Prominent; , 20-50% , 15-30mm, Prominent; 
	Heavy clay; Moderate grade of structure, Angular blocky; Moderately moist; Firm consistence; 
	0-2%, medium gravelly, 6-20mm, angular, Substrate material, coarse fragments; Field pH 4 (pH 
	meter); Diffuse change to - 
	3.66 - 3.81 m	Red (10R4/6-Moist); , 2.5Y62, 20-50% , 15-30mm, Prominent; , 20-50% , 15-30mm, Prominent; 
	Heavy clay; Moderate grade of structure, Angular blocky; Firm consistence; 20-50%, angular, 
	Substrate material, coarse fragments; Field pH 4 (pH meter); 
	Morphological Notes
	Observation Notes
	0-7CM GRANULAR GRADING TO STRONG 10-20MM BLOCKY STRUCTURE:                                                              
	Site Notes
	BUNGUNYA

	Project Name:	BL
	Project Code:	BL	Site ID:	B332	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	6.3H	 0.04B
	0.07 - 0.23	6.7H	 0.09B
	0.23 - 0.46	4.9H	 0.42B
	0.46 - 0.91	4.4H	 0.48B
	0.91 - 1.6	4.3H	 0.54B
	1.6 - 2.08	4.3H	 0.4B
	2.08 - 2.49	4.3H	 0.38B
	2.49 - 3	4.1H	 0.47B
	3.05 - 3.66	4H	 0.74B	 2.4K	 11.2	 0.28	 2.8	 28.4J	9.86
	3.66 - 3.81	4H	 0.75B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07	 1.46E	 17C	 0.036F	1.40	 1	 2C	 37	 14	 44
	0.07 - 0.23	1.50
	0.23 - 0.46	 0.43E	1.40	 0	 1C	 30	 12	 54
	0.46 - 0.91	1.40
	0.91 - 1.6	 0.21E	 0.012F	1.40	 0	 1C	 34	 14	 51
	1.6 - 2.08
	2.08 - 2.49	 6C	 50	 11	 34
	2.49 - 3
	3.05 - 3.66	 0.013F	 1	 3C	 26	 14	 59
	3.66 - 3.81	 35	 11C	 21	 14	 56
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07	 0.39C	 0.22C
	0.07 - 0.23	 0.43C	 0.27C
	0.23 - 0.46	 0.43C	 0.25C
	0.46 - 0.91	 0.43C	 0.28C
	0.91 - 1.6	 0.44C	 0.25C
	1.6 - 2.08
	2.08 - 2.49
	2.49 - 3
	3.05 - 3.66
	3.66 - 3.81

	Project Name:	BL
	Project Code:	BL	Site ID:	B332	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate