Project Name:	BOB
	Project Code:	BOB	Site ID:	B493	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R. Paton	Locality:
	Date Desc.:	09/04/62	Elevation:	 40 metres
	Map Ref.:	Sheet No. : 9542   1:100000	Rainfall:	864
	Northing/Long.:	153.008333333333	Runoff:	Moderately rapid
	Easting/Lat.:	-27.8375	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Jm	Substrate Material:	Soil pit, 0.56 m deep,Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	15 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Brown Sodosol     	Principal Profile Form:	Dy3.21
	ASC Confidence:	Great Soil Group:	Soloth
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus crebra, Eucalyptus tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Very dark brown (10YR2/2-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, Angular 
	blocky; Moist; Very weak consistence; Field pH 5.8 (pH meter); Clear change to - 
	A2	0.05 - 0.15 m	Dark greyish brown (10YR4/2-Moist); ; Loamy sand; Massive grade of structure; Moist; Very 
	weak consistence; Field pH 5.7 (pH meter); Clear change to - 
	B2	0.15 - 0.3 m	Strong brown (7.5YR5/8-Moist); , 10YR64; , 10YR52; Sandy medium clay; Moderate grade of 
	structure, 100-200 mm, Columnar; Moderate grade of structure, 20-50 mm, Angular blocky; Wet;
	 Firm consistence; Field pH 6 (pH meter); Gradual change to - 
	B2	0.3 - 0.56 m	Red (2.5YR5/8-Moist); , 10YR66; , 10YR63; Sandy medium clay; Moderate grade of structure, 
	20-50 mm, Angular blocky; Wet; Firm consistence; Field pH 5.9 (pH meter); Abrupt change to - 
	C	0.56 - 0.7 m	; 
	Morphological Notes
	C	Weathered sandstone.
	Observation Notes
	Site Notes
	BOONAH

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B493	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.8H	 0.01B	 4.6K	 1.6	 0.35	 0.04	 5.8D
	0.05 - 0.15	5.7H	 0.01B	 1.2K	 0.78	 0.2	 0.1	 3.1D
	0.15 - 0.3	6H	 0.02B	 1.1K	 8.2	 0.25	 1.5	 3.8D
	0.3 - 0.56	5.9H	 0.05B	 0.62K	 9.2	 0.22	 2.4	 2.5D
	0.56 - 0.86
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 2.07A	 14C	 0.019F	 0.2B	 0	 42C	 31	 14	 8
	0.05 - 0.15	 0.013F	 45C	 31	 17	 5
	0.15 - 0.3	 0.009F	 0	 30C	 23	 14	 32
	0.3 - 0.56	 0.008F	 0	 30C	 24	 13	 33
	0.56 - 0.86
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.15
	0.15 - 0.3
	0.3 - 0.56
	0.56 - 0.86

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B493	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded