Project Name:	BOB
	Project Code:	BOB	Site ID:	B508	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R. Paton	Locality:
	Date Desc.:	19/11/63	Elevation:	 110 metres
	Map Ref.:	Sheet No. : 9442   1:100000	Rainfall:	914
	Northing/Long.:	152.536111111111	Runoff:	Rapid
	Easting/Lat.:	-27.8572222222222	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Jw	Substrate Material:	Soil pit, 0.91 m deep,Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Lower-slope	Relief:	213 metres
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Natric Yellow Kurosol     	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	Soloth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Tall Strata - Tree, , Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.03 m	Brown (7.5YR5/2-Moist); ; Fine sandy loam; Massive grade of structure; Moderately moist; 
	Weak consistence; 0-2%, coarse gravelly, 20-60mm, Quartz, coarse fragments; Field pH 6.1 
	(pH meter); Many, fine (1-2mm) roots; Sharp change to - 
	A2	0.03 - 0.13 m	Light yellowish brown (10YR6/4-Moist); White (10YR8/2-Dry); , 10YR62; Fine sandy loam; 
	Massive grade of structure; Moderately moist; Weak consistence; 0-2%, medium gravelly, 6-
	20mm, Quartz, coarse fragments; Field pH 5.5 (pH meter); Many, fine (1-2mm) roots; Sharp 
	change to - 
	B2	0.13 - 0.18 m	Brown (7.5YR5/4-Moist); , 7.5YR56; , 10YR51; Medium heavy clay; Moderate grade of 
	structure, 5-10 mm, Angular blocky; Wet; Field pH 5.4 (pH meter); Common, fine (1-2mm) roots; 
	Gradual change to - 
	B2	0.18 - 0.53 m	Light yellowish brown (10YR6/4-Moist); , 2.5Y62; Heavy clay; Moderate grade of structure, 5-
	10 mm, Angular blocky; Wet; Field pH 5 (pH meter); Few, fine (1-2mm) roots; Gradual change to 
	B2	0.53 - 0.69 m	Yellowish brown (10YR5/5-Moist); , 10YR63; Medium clay; Moderate grade of structure, 5-10 
	mm, Angular blocky; Wet; Field pH 4.9 (pH meter); Few, fine (1-2mm) roots; Gradual change to -
	B3	0.69 - 0.91 m	Yellow (10YR7/6-Moist); , 2.5Y62; Light medium clay; Weak grade of structure, 5-10 mm, 
	Angular blocky; Wet; 2-10%, Sandstone, coarse fragments; Few (2 - 10 %), , , ; Field pH 5 (pH 
	Morphological Notes
	Observation Notes
	BELOW .91M WEATHERING SANDSTONE IN SITU:                                                                                
	Site Notes
	COLEYVILLE

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B508	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	6.1H	 0.03B
	0.03 - 0.13	5.5H	 0.02B	 1.5K	 4.2	 0.41	 0.7	 8.5D
	0.13 - 0.18	5.4H	 0.04B
	0.18 - 0.53	5H	 0.13B	 1.1K	 12.9	 0.3	 4.9	 23D
	0.53 - 0.69	4.9H	 0.17B
	0.69 - 0.91	5H	 0.15B	 1.1K	 12.4	 0.17	 6.6	 13.3D
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03	 2.91A	 0.03F	 0.208B	 8C	 47	 20	 19
	0.03 - 0.13	 0.67A	 4C	 0.014F	 0.054B	1.40	 7C	 47	 24	 22
	0.13 - 0.18	1.50
	0.18 - 0.53	 0.014F	1.50	 2C	 21	 17	 62
	0.53 - 0.69	1.60
	0.69 - 0.91	 0	 14C	 19	 26	 43
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.13	 0.2C	 0.09C
	0.13 - 0.18	 0.41C	 0.28C
	0.18 - 0.53	 0.47C	 0.32C
	0.53 - 0.69	 0.41C	 0.34C
	0.69 - 0.91

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B508	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	MIN_EC	Exchange Capacity - Minerology
	MIN_NR_K2O	Kaolin minerals
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate
	P3B_VL_15	15 BAR Moisture m3/m3 - Volumetric using pressure plate
	XRD_C_Fd	Feldspar - X-Ray Diffraction
	XRD_C_Il	Illite - X-Ray Diffraction
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Mm	Montmorillonite - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction