Project Name:	BOB
	Project Code:	BOB	Site ID:	B514	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R. Paton	Locality:
	Date Desc.:	07/11/63	Elevation:	 76 metres
	Map Ref.:	Sheet No. : 9442   1:100000	Rainfall:	864
	Northing/Long.:	152.809444444445	Runoff:	Moderately rapid
	Easting/Lat.:	-27.9266666666667	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Jm	Substrate Material:	Soil pit, 0.84 m deep,Sandstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	61 metres
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Natric Grey Kurosol     	Principal Profile Form:	Dy3.41
	ASC Confidence:	Great Soil Group:	Soloth
	No analytical data are available but confidence is fair.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.06 m	Dark brown (7.5YR3/2-Moist); ; Loamy sand; Weak grade of structure, 10-20 mm, Granular; 
	Dry; Very weak consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 
	6.2 (pH meter); Many, fine (1-2mm) roots; Clear change to - 
	A21	0.06 - 0.23 m	Very pale brown (10YR7/3-Moist); ; Sand; Single grain grade of structure; Dry; Loose 
	consistence; 2-10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.2 (pH meter); 
	Few, fine (1-2mm) roots; Gradual change to - 
	A22	0.23 - 0.43 m	Pink (5YR8/4-Moist); ; Sand; Single grain grade of structure; Dry; Very weak consistence; 2-
	10%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 6.6 (pH meter); Few, fine (1-
	2mm) roots; Sharp change to - 
	B2	0.43 - 0.84 m	Light brownish grey (2.5Y6/2-Moist); , 10R46, 20-50% , 30-mm, Prominent; , 7.5YR68, 20-50% ,
	 30-mm, Prominent; Heavy clay; Moderate grade of structure, 50-100 mm, Prismatic; Moderate 
	grade of structure, 10-20 mm, Angular blocky; Dry; Very strong consistence; 0-2%, fine 
	gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.4 (pH meter); Few, fine (1-2mm) roots; 
	Clear change to - 
	C	0.84 - 0.94 m	; Field pH 5.4 (pH meter); 
	Morphological Notes
	C	VPB(10YR8/3) & RY(7.5YR7/8) weathered sandstone.
	Observation Notes
	0-6CM POROUS GRANULAR STRUCTURE.                                                                                        
	Site Notes
	WYARALONG

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B514	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.2H	 0.02B
	0.06 - 0.23	6.2H	 0.01B
	0.23 - 0.43	6.6H	 0.01B
	0.43 - 0.84	5.4H	 0.03B
	0.84 - 0.94	5.4H	 0.03B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 6C	 0.008F
	0.06 - 0.23
	0.23 - 0.43
	0.43 - 0.84
	0.84 - 0.94
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.23
	0.23 - 0.43
	0.43 - 0.84
	0.84 - 0.94

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B514	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded