Project Name:	BOB
	Project Code:	BOB	Site ID:	B515	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	R. Paton	Locality:
	Date Desc.:	08/11/63	Elevation:	 67 metres
	Map Ref.:	Sheet No. : 9442   1:100000	Rainfall:	864
	Northing/Long.:	152.810555555556	Runoff:	Slow
	Easting/Lat.:	-27.9277777777778	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Jm	Substrate Material:	Auger boring, 1.8 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Pediment
	Morph. Type:	Lower-slope	Relief:	76 metres
	Elem. Type:	Footslope	Slope Category:	No Data
	Slope:	0.87 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Hypernatric Brown Sodosol     	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Brown (7.5YR5/2-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, Platy; Dry; Weak 
	consistence; Field pH 5.8 (pH meter); Many, fine (1-2mm) roots; Abrupt change to - 
	A21	0.08 - 0.3 m	Very pale brown (10YR7/3-Moist); ; Loamy sand; Massive grade of structure; Dry; Very weak 
	consistence; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 6 
	(pH meter); Few, fine (1-2mm) roots; Gradual change to - 
	A22	0.3 - 0.41 m	White (10YR8/1-Moist); ; Coarse sandy loam; Massive grade of structure; Dry; Weak 
	consistence; Common (10 - 20 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 7 
	(pH meter); Few, fine (1-2mm) roots; Abrupt change to - 
	B2	0.41 - 0.69 m	Strong brown (7.5YR5/6-Moist); , 10YR63; Medium clay; Moderate grade of structure, 20-50 
	mm, Angular blocky; Dry; Very firm consistence; Common (10 - 20 %), Ferromanganiferous, 
	Medium (2 -6 mm), Nodules; Field pH 7.2 (pH meter); Few, fine (1-2mm) roots; Gradual change 
	B2	0.69 - 1.09 m	Yellowish brown (10YR5/4-Moist); , 2.5Y72; Sandy medium clay; Moderate grade of structure, 
	20-50 mm, Angular blocky; Moderately moist; Firm consistence; Few (2 - 10 %), 
	Ferromanganiferous, Medium (2 -6 mm), Nodules; Field pH 7.6 (pH meter); Gradual change to - 
	B3	1.09 - 1.37 m	Brownish yellow (10YR6/6-Moist); , 10YR82; , 10YR63; Sandy medium clay; Weak grade of 
	structure, 20-50 mm, Angular blocky; Moderately moist; Firm consistence; Field pH 8.1 (pH 
	meter); Gradual change to - 
	B3	1.37 - 1.83 m	Very pale brown (10YR7/4-Moist); , 10YR54; , 2.5Y82; Sandy medium clay; Weak grade of 
	structure, 20-50 mm, Angular blocky; Moderately moist; Firm consistence; Field pH 8.4 (pH 
	meter); Gradual change to - 
	C	1.83 - 2.28 m	Brownish yellow (10YR6/6-Moist); , 10YR61; , 10YR81; Sandy clay loam; Massive grade of 
	structure; Moderately moist; Firm consistence; Field pH 8.7 (pH meter); Gradual change to - 
	C	2.28 - 2.43 m	Yellowish brown (10YR5/8-Moist); , 10YR81; Sandy clay loam (Light); Massive grade of 
	structure; Moderately moist; Firm consistence; Few (2 - 10 %), Ferromanganiferous, Medium (2 
	-6 mm), Nodules; Field pH 8.6 (pH meter); 
	Morphological Notes
	Observation Notes

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B515	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0-8CM POROUS GRANULAR STRUCTURE.                                                                                        
	Site Notes
	WYARALONG

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B515	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.8H	 0.02B	 2.2K	 1.1	 0.22	 0.12	 6.2D
	0.08 - 0.3	6H	 0.01B
	0.3 - 0.41	7H	 0.02B
	0.41 - 0.69	7.2H	 0.11B	 4.1K	 6.4	 0.18	 6.7	 2.4D
	0.69 - 1.09	7.6H	 0.17B
	1.09 - 1.37	8.1H	 0.16B	 2.6K	 6.5	 0.12	 7	 0D
	1.37 - 1.83	8.4H	 0.15B
	1.83 - 2.28	8.7H	 0.11B
	2.28 - 2.43	8.6H	 0.11B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 1.45A	 6C	 0.017F	 0.126B	 39C	 26	 22	 9
	0.08 - 0.3
	0.3 - 0.41	 0.08A	 15	 48C	 23	 18	 10
	0.41 - 0.69	 0.006F	 13	 36C	 13	 9	 44
	0.69 - 1.09
	1.09 - 1.37	 0.1C	 38C	 28	 10	 25
	1.37 - 1.83
	1.83 - 2.28	 0.1C
	2.28 - 2.43
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.3
	0.3 - 0.41
	0.41 - 0.69
	0.69 - 1.09
	1.09 - 1.37
	1.37 - 1.83
	1.83 - 2.28
	2.28 - 2.43

	Project Name:	BOB
	Project Code:	BOB	Site ID:	B515	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded