Project Name:	CB
	Project Code:	CB	Site ID:	B380	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	24/04/59	Elevation:	 108 metres
	Map Ref.:	Sheet No. : 9246   1:100000	Rainfall:	762
	Northing/Long.:	151.716111111111	Runoff:	Moderately rapid
	Easting/Lat.:	-25.6122222222222	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Ra	Substrate Material:	Auger boring, 1.6 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous Crusty Black Vertosol     	Principal Profile Form:	Ug5.4
	ASC Confidence:	Great Soil Group:	Black earth
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Very dark grey (10YR3/1-Moist); ; Light clay; Weak grade of structure, 20-50 mm, Angular 
	blocky; Massive grade of structure; Dry; Very firm consistence; 2-10%, fine gravelly, 2-6mm, 
	coarse fragments; Few (2 - 10 %), Calcareous, , Nodules; Field pH 8 (pH meter); Gradual 
	B2	0.15 - 0.3 m	Black (10YR2/1-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular blocky; 
	Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, coarse fragments; Few (2 - 10 %), 
	Calcareous, , Nodules; Field pH 8.3 (pH meter); Gradual change to - 
	B2	0.46 - 0.61 m	Black (10YR2/1-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular blocky; 
	Moist; Firm consistence; Few (2 - 10 %), Calcareous, , Nodules; Field pH 8.5 (pH meter); 
	Gradual change to - 
	B2	0.76 - 0.91 m	Dark greyish brown (10YR4/2-Moist); ; Light medium clay; Strong grade of structure, Angular 
	blocky; Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, Substrate material, coarse 
	fragments; Few (2 - 10 %), Calcareous, , Nodules; Field pH 8.7 (pH meter); Diffuse change to - 
	B2	1.07 - 1.22 m	Dark greyish brown (10YR4/2-Moist); ; Medium clay; Strong grade of structure, Angular blocky; 
	Moist; Firm consistence; 2-10%, fine gravelly, 2-6mm, Substrate material, coarse fragments; 
	Common (10 - 20 %), Calcareous, , Nodules; Field pH 8.7 (pH meter); Diffuse change to - 
	2B2b	1.37 - 1.52 m	Brown (7.5YR4/2-Moist); ; Medium clay; Moderate grade of structure, Angular blocky; Moist; 
	Firm consistence; 10-20%, medium gravelly, 6-20mm, Substrate material, coarse fragments; 
	Very few (0 - 2 %), Calcareous, , Nodules; Field pH 8.6 (pH meter); 
	Morphological Notes
	Observation Notes
	C.DEM. INDICATES LAYERED SOIL AT 137CM:                                                                                 
	Site Notes
	CENTRAL BURNET

	Project Name:	CB
	Project Code:	CB	Site ID:	B380	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	8H	 0.06B	 21.4K	 4	 0.94	 0.26
	0.15 - 0.3	8.3H	 0.05B	 25.3K	 4.5	 0.7	 0.34	 32.6J	1.04
	0.46 - 0.61	8.5H	 0.05B
	0.76 - 0.91	8.7H	 0.05B	 21.8K	 5.6	 0.46	 0.74
	1.07 - 1.22	8.7H	 0.05B
	1.37 - 1.52	8.6H	 0.06B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	 2C	 2.25E	 140C	 0.042F	 0.18B	1.40	 8	 9C	 18	 24	 46
	0.15 - 0.3	 2.6C	 1.71E	 150C	 0.039F	 0.13B	1.40	 3	 10C	 21	 22	 44
	0.46 - 0.61	 1.9C	 1.44E	 0.033F	 0.1B
	0.76 - 0.91	 8.2C	 0.8E	 0.051F	 0.06B	 2	 15C	 20	 18	 39
	1.07 - 1.22	 2.5C	 0.61E	 0.027F	 0.04B
	1.37 - 1.52	 1.4C	 0.79E	 0.028F	 0.05B
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15	 0.43C
	0.15 - 0.3	 0.4C
	0.46 - 0.61
	0.76 - 0.91
	1.07 - 1.22
	1.37 - 1.52

	Project Name:	CB
	Project Code:	CB	Site ID:	B380	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate