Project Name:	CB
	Project Code:	CB	Site ID:	B388	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.J. de Mooy	Locality:
	Date Desc.:	27/04/59	Elevation:	 107 metres
	Map Ref.:	Sheet No. : 9246   1:100000	Rainfall:	762
	Northing/Long.:	151.586666666667	Runoff:	Moderately rapid
	Easting/Lat.:	-25.6227777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Rg	Substrate Material:	Auger boring, 1.2 m deep,Igneous rock 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Surface crust
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Epicalcareous-Endohypersodic Crusty Grey Vertosol     	Principal Profile Form:	Ug5.28
	ASC Confidence:	Great Soil Group:	Grey clay
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus species, Acacia harpophylla
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Very dark grey (10YR3/1-Moist); ; Medium clay; Moderate grade of structure, Angular blocky; 
	Moist; Firm consistence; 0-2%, medium gravelly, 6-20mm, subrounded, Quartz, coarse 
	fragments; Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 8.5 (pH meter); Clear 
	change to - 
	B2	0.08 - 0.23 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium clay; Strong grade of structure, Angular blocky; 
	Moist; Firm consistence; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; 
	Few (2 - 10 %), Calcareous, , Soft segregations; Field pH 8.6 (pH meter); Gradual change to - 
	B2	0.23 - 0.38 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium clay; Strong grade of structure, Angular blocky; 
	Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Few (2 - 10 %),
	 Calcareous, , Soft segregations; Field pH 8.9 (pH meter); Gradual change to - 
	B2	0.46 - 0.61 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium clay; Strong grade of structure, Angular blocky; 
	Moist; Moderately plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field pH 9 (pH 
	meter); Gradual change to - 
	B2	0.61 - 0.76 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium clay; Moderate grade of structure, Angular 
	blocky; Moist; Moderately plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field 
	pH 9 (pH meter); Gradual change to - 
	B2	0.76 - 0.91 m	Dark greyish brown (2.5Y4/2-Moist); ; Medium clay; Moderate grade of structure, Angular 
	blocky; Moist; Moderately plastic; Common (10 - 20 %), Calcareous, , Soft segregations; Field 
	pH 9 (pH meter); Diffuse change to - 
	BC	0.91 - 1.07 m	Greyish brown (2.5Y5/2-Moist); ; Heavy clay; , Angular blocky; Moist; Moderately plastic; Few 
	(2 - 10 %), Calcareous, , Soft segregations; Field pH 9.2 (pH meter); Diffuse change to - 
	C	1.22 - 1.37 m	Pale yellow (2.5Y7/4-Moist); ; Heavy clay; Moist; Moderately plastic; Few (2 - 10 %), 
	Calcareous, , Soft segregations; Field pH 9.4 (pH meter); Diffuse change to - 
	C	1.37 - 1.52 m	Pale yellow (2.5Y7/4-Moist); ; Heavy clay; Moist; Moderately plastic; Few (2 - 10 %), 
	Calcareous, , Soft segregations; Field pH 9.4 (pH meter); Diffuse change to - 

	Project Name:	CB
	Project Code:	CB	Site ID:	B388	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	C	1.68 - 1.83 m	Pale yellow (2.5Y8/4-Moist); , 10YR66; Heavy clay; Moist; Moderately plastic; Field pH 9.4 (pH 
	meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	CENTRAL BURNET

	Project Name:	CB
	Project Code:	CB	Site ID:	B388	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	8.5H	 0.07B	 24.2K	 11.6	 0.66	 0.38
	0.08 - 0.23	8.6H	 0.07B
	0.23 - 0.38	8.9H	 0.09B	 18.8K	 20.7	 0.3	 2.3
	0.46 - 0.61	9H	 0.19B
	0.61 - 0.76	9H	 0.24B
	0.76 - 0.91	9H	 0.28B	 5.8K	 21.5	 0.26	 5.5
	0.91 - 1.07	9.2H	 0.28B
	1.22 - 1.37	9.4H	 0.26B
	1.37 - 1.52	9.4H	 0.24B
	1.68 - 1.83	9.4H	 0.2B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 4.5C	 1E	 4C	 0.02F	 0.12B	1.20	 5C	 15	 17	 58
	0.08 - 0.23
	0.23 - 0.38	 4.6C	 0.7E	 2C	 0.013F	 0.07B	1.30	 1	 6C	 14	 17	 58
	0.46 - 0.61
	0.61 - 0.76
	0.76 - 0.91	 16.2C	 3	 5C	 13	 14	 54
	0.91 - 1.07
	1.22 - 1.37
	1.37 - 1.52
	1.68 - 1.83	 3C
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08	 0.46C
	0.08 - 0.23
	0.23 - 0.38	 0.43C
	0.46 - 0.61
	0.61 - 0.76
	0.76 - 0.91
	0.91 - 1.07
	1.22 - 1.37
	1.37 - 1.52
	1.68 - 1.83

	Project Name:	CB
	Project Code:	CB	Site ID:	B388	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_VL_01	0.1 BAR Moisture m3/m3 - Volumetric using suction plate