Project Name:	CL
	Project Code:	CL	Site ID:	B179	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	09/02/52	Elevation:	 24 metres
	Map Ref.:	Sheet No. : 9143   1:100000	Rainfall:	1143
	Northing/Long.:	151.986111111111	Runoff:	Moderately rapid
	Easting/Lat.:	-27.1802777777778	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	R-Jo	Substrate Material:	Auger boring, 2 m deep,Porous, Sandstone 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	40 metres
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Magnesic Yellow Chromosol     	Principal Profile Form:	Dy5.41
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - Imperata cylindrica, Pteridium esculentum
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Grey (10YR5/1-Moist); ; Loamy sand; Weak grade of structure, 2-5 mm, Granular; Dry; Loose 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Very few (0 - 2 
	%), Ferruginous, Medium (2 -6 mm), Nodules; Field pH 6 (pH meter); Common, fine (1-2mm) 
	roots; Clear change to - 
	A2	0.1 - 0.28 m	Light olive grey (5Y6/2-Moist); ; Clayey sand; Massive grade of structure; Dry; Very weak 
	consistence; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Very few (0 - 2 
	%), Ferruginous, Medium (2 -6 mm), Nodules; Field pH 6.1 (pH meter); Few, fine (1-2mm) roots; 
	Gradual change to - 
	A3	0.28 - 0.61 m	Pale yellow (2.5Y7/4-Moist); , 10YR61; Clayey sand; Massive grade of structure; Moderately 
	moist; Very weak consistence; Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Nodules; 
	Field pH 6.2 (pH meter); Gradual change to - 
	B1	0.61 - 0.84 m	Brownish yellow (10YR6/6-Moist); , 2.5YR48; Sandy clay loam; Massive grade of structure; 
	Moist; Very weak consistence; Very few (0 - 2 %), Ferruginous, Coarse (6 - 20 mm), Nodules; 
	Field pH 5.9 (pH meter); Gradual change to - 
	B21	0.84 - 1.37 m	Brownish yellow (10YR6/6-Moist); , 5YR56; Medium clay; Moderate grade of structure, Angular
	 blocky; Moist; Weak consistence; 0-2%, fine gravelly, 2-6mm, rounded, Quartz, coarse 
	fragments; Many (20 - 50 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 5.8 (pH 
	meter); Diffuse change to - 
	B22	1.37 - 1.9 m	Reddish yellow (7.5YR7/8-Moist); , 10R36; , 5Y81; Heavy clay; Moderate grade of structure, 
	Angular blocky; Moist; Weak consistence; 0-2%, medium gravelly, 6-20mm, subrounded, 
	Quartz, coarse fragments; Few (2 - 10 %), Ferruginous, Coarse (6 - 20 mm), Nodules; Field pH 
	5.9 (pH meter); Diffuse change to - 
	B23	2.01 - 2.46 m	White (5Y8/1-Moist); , 10R46; , 10YR68; Heavy clay; Moderate grade of structure, Angular 
	blocky; Moist; Weak consistence; Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Nodules; 
	Field pH 5.7 (pH meter); 
	Morphological Notes
	Observation Notes
	UPPER 4CM POSSIBLY OLDER ALLUVIUM ON TRUNCATED PROFILE:ALTERED LATERITISED SANDSTONE AT 5.6M                    

	Project Name:	CL
	Project Code:	CL	Site ID:	B179	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Notes
	DECEPTION BAY

	Project Name:	CL
	Project Code:	CL	Site ID:	B179	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6H	 0.012B	 1.6K	 0.6	 0.07	 0.05	 5.33D	 7.65E
	0.1 - 0.28	6.1H	 0.007B
	0.28 - 0.61	6.2H	 0.007B
	0.61 - 0.84	5.9H	 0.007B	 0.3K	 1.1	 0.12	 0.07	 2.57D	 4.16E
	0.84 - 1.37	5.8H	 0.011B	 0.3K	 3.3	 0.04	 0.22	 6.7D	 10.6E
	1.37 - 1.9	5.9H	 0.006B
	2.01 - 2.46	5.7H	 0.006B	 0.3K	 3.6	 0.04	 0.35	 4.65D	 8.8E
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.41E	 6C	 0.006F	 0.07B	 3	 53C	 31	 8	 8
	0.1 - 0.28	 0.003F	 0.015B	 2	 51C	 34	 9	 6
	0.28 - 0.61	 0.016B	 0	 48C	 33	 9	 10
	0.61 - 0.84	 0.016B	 0	 42C	 29	 9	 19
	0.84 - 1.37	 0.007F	 0.018B	 46	 22C	 15	 11	 54
	1.37 - 1.9
	2.01 - 2.46	 0	 19C	 14	 15	 54
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.28
	0.28 - 0.61
	0.61 - 0.84
	0.84 - 1.37
	1.37 - 1.9
	2.01 - 2.46

	Project Name:	CL
	Project Code:	CL	Site ID:	B179	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded