Project Name:	CL
	Project Code:	CL	Site ID:	B182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	G.D. Hubble	Locality:
	Date Desc.:	10/12/52	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 9344   1:100000	Rainfall:	1397
	Northing/Long.:	152.988611111111	Runoff:	Slow
	Easting/Lat.:	-26.9111111111111	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Soil pit, 1.1 m deep,Porous, Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Rises
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic Dermosolic Redoxic Hydrosol     	Principal Profile Form:	Gn3.91
	ASC Confidence:	Great Soil Group:	Humic gley
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation:
	Tall Strata - Sod grass, <0.25m, Closed or dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11g	0 - 0.1 m	Very dark grey (10YR3/1-Moist); Grey (10YR5/1-Dry); ; Clay loam (Fibric); Strong grade of 
	structure, 5-10 mm, Granular; Moist; Weak consistence; Field pH 5.3 (pH meter); Abundant, fine 
	(1-2mm) roots; Clear change to - 
	A12g	0.1 - 0.2 m	Very dark grey (10YR3/1-Moist); Grey (10YR5/1-Dry); ; Light clay (Fibric); Strong grade of 
	structure, 10-20 mm, Subangular blocky; Moderately moist; Weak consistence; Field pH 5.4 (pH 
	meter); Abundant, fine (1-2mm) roots; Gradual change to - 
	A13g	0.2 - 0.33 m	Dark grey (10YR4/1-Moist); Grey (10YR5/1-Dry); , 10YR71; Medium heavy clay; Strong grade 
	of structure, 100-200 mm, Prismatic; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry;
	 Strong consistence; Field pH 5.6 (pH meter); Many, fine (1-2mm) roots; Gradual change to - 
	Bg	0.33 - 0.46 m	Light grey (10YR7/2-Moist); White (10YR8/1-Dry); , 10YR66; Silty medium clay (Light); Strong 
	grade of structure, 100-200 mm, Prismatic; Common (1-5 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Strong consistence; Field pH 5.8 (pH meter); Gradual change to - 
	Bg	0.46 - 0.66 m	White (10YR8/1-Dry); , 10YR78; Silty clay loam; Weak grade of structure, 100-200 mm, 
	Prismatic; Dry; Firm consistence; Few (2 - 10 %), Ferruginous, , Nodules; Field pH 5.6 (pH 
	meter); Diffuse change to - 
	Bg	0.66 - 0.97 m	White (10YR8/1-Dry); , 2.5Y84; , 10YR76; Fine sandy clay loam; Massive grade of structure; 
	Moist; Very weak consistence; Field pH 5.8 (pH meter); Diffuse change to - 
	D	1.02 - 1.22 m	White (2.5Y8/0-Dry); , 10YR68; , 10R48; Medium clay; Massive grade of structure; Moist; Very 
	plastic; Field pH 5.6 (pH meter); 
	Morphological Notes
	Observation Notes
	0-46CM RUSTY ROOT MARKINGS : FIG.41.1 H.A.S. P387                                                                       
	Site Notes
	BEERBURRUM

	Project Name:	CL
	Project Code:	CL	Site ID:	B182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.3H	 0.026B	 5.4K	 3	 0.52	 0.41	 44.8D	 54.2E
	0.1 - 0.2	5.4H	 0.016B
	0.2 - 0.33	5.6H	 0.011B	 3.7K	 3.8	 0.31	 0.49	 25D	 33.3E
	0.33 - 0.46	5.8H	 0.007B	 1.8K	 2.7	 0.14	 0.26	 11D	 15.9E
	0.46 - 0.66	5.6H	 0.008B	 1.1K	 1.4	 0.1	 0.15	 7D	 9.8E
	0.66 - 0.97	5.8H	 0.007B
	1.02 - 1.22	5.6H	 0.012B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 8.05E	 6C	 0.045F	 0.603B	 0	 1C	 7	 21	 52
	0.1 - 0.2	 4.63E	 0.373B	 0	 1C	 16	 26	 50
	0.2 - 0.33	 2.63E	 0.017F	 0.208B	 0	<1C	 14	 26	 56
	0.33 - 0.46	 0.81E	 0.059B	 0	 2C	 23	 33	 40
	0.46 - 0.66	 0.009F	 0.027B	 0	 3C	 32	 36	 29
	0.66 - 0.97	 0	 5C	 37	 38	 19
	1.02 - 1.22	 0	 3C	 28	 29	 41
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.33
	0.33 - 0.46
	0.46 - 0.66
	0.66 - 0.97
	1.02 - 1.22

	Project Name:	CL
	Project Code:	CL	Site ID:	B182	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR	Sum of Ex. cations + Ex. acidity - Not recorded
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded