Project Name:	CL
	Project Code:	CL	Site ID:	B339	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	06/11/57	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 9544   1:100000	Rainfall:	1524
	Northing/Long.:	153.015277777778	Runoff:	Very slow
	Easting/Lat.:	-26.8444444444444	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Auger boring, 2 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	0 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melacic-Bleached Chomosolic Oxyaquic Hydrosol     	Principal Profile Form:	Dg4.81
	ASC Confidence:	Great Soil Group:	Humic gley
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - , , . *Species includes - Xanthorrhoea species
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Closed or dense. *Species includes - Trigonella suavissima, Melaleuca decora, Eucalyptus 
	robusta
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.18 m	Black (10YR2/1-Moist); ; Loam (Fibric); Moderate grade of structure, 2-5 mm, Granular; Moist; 
	Weak consistence; Field pH 5.2 (pH meter); Abundant, fine (1-2mm) roots; Gradual change to - 
	A12	0.18 - 0.52 m	Very dark grey (10YR3/1-Moist); ; Loam (Fibric); Strong grade of structure, 5-10 mm, 
	Polyhedral; Moist; Weak consistence; Field pH 5.2 (pH meter); Many, fine (1-2mm) roots; 
	A13	0.58 - 0.76 m	Very dark grey (10YR3/1-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, Angular 
	blocky; Moist; Very weak consistence; Field pH 5.1 (pH meter); Many, fine (1-2mm) roots; 
	Gradual change to - 
	A14	0.76 - 1.07 m	Dark grey (10YR4/1-Moist); ; Clayey sand; Weak grade of structure, 5-10 mm, Angular blocky; 
	Moist; Very weak consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 
	5.3 (pH meter); Common, very fine (0-1mm) roots; Gradual change to - 
	A2	1.12 - 1.3 m	White (10YR8/1-Moist); ; Sand; Massive grade of structure; Moist; Very weak consistence; 0-
	2%, fine gravelly, 2-6mm, Quartz, coarse fragments; Field pH 5.9 (pH meter); Few, very fine (0-
	1mm) roots; Sharp change to - 
	B2	1.3 - 1.57 m	Light grey (10YR7/2-Moist); ; Sandy medium clay; Weak grade of structure, Prismatic; Massive 
	grade of structure; Moist; Firm consistence; 0-2%, fine gravelly, 2-6mm, Quartz, coarse 
	fragments; Field pH 5.5 (pH meter); Few, very fine (0-1mm) roots; Gradual change to - 
	B3	1.65 - 1.93 m	Light grey (10YR7/1-Moist); , 7.5YR54, 10-20% , 15-30mm, Faint; , 10-20% , 15-30mm, Faint; 
	Sandy clay loam; Massive grade of structure; Moist; Weak consistence; 0-2%, fine gravelly, 2-
	6mm, subrounded, Quartz, coarse fragments; Field pH 5.5 (pH meter); Gradual change to - 
	B3	1.98 - 2.13 m	Light grey (10YR7/1-Moist); , 10YR61, 10-20% , 15-30mm, Faint; , 10-20% , 15-30mm, Faint; 
	Sandy medium clay; Massive grade of structure; Wet; Moderately plastic; 0-2%, fine gravelly, 2-
	6mm, subrounded, Quartz, coarse fragments; Field pH 5.7 (pH meter); Gradual change to - 

	Project Name:	CL
	Project Code:	CL	Site ID:	B339	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	BC	2.13 - 2.36 m	Light grey (10YR7/1-Moist); , 10YR61, 10-20% , 15-30mm, Faint; , 10-20% , 15-30mm, Faint; 
	Clayey coarse sand; Massive grade of structure; Wet; Moderately plastic; 2-10%, medium 
	gravelly, 6-20mm, subrounded, Quartz, coarse fragments; Field pH 5.7 (pH meter); 
	Morphological Notes
	Observation Notes
	WATER TABLE NEAR SURFACE FOR MOST OF THE YEAR: 0-193CM PROMINENT OCHEROUS FLECKING: CLAY BALLS IN 
	LOWER A2:             
	Site Notes
	BEERWAH

	Project Name:	CL
	Project Code:	CL	Site ID:	B339	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.18	5.2H	 0.02C	 0.02K	 0.16	 0.1	 0.08	 23.4J	0.34
	0.18 - 0.52	5.2H	 0.02C
	0.58 - 0.76	5.1H	 0.01C
	0.76 - 1.07	5.3H	 0.01C
	1.12 - 1.3	5.9H	 0.01C
	1.3 - 1.57	5.5H	 0.01C	 0.2K	 0.7	 0.04	 0.16	 8.2J	1.95
	1.65 - 1.93	5.5H	 0.01C
	1.98 - 2.13	5.7H	 0.01C
	2.13 - 2.36	5.7H	 0.01C
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.18	 4.86E	 2C	 0.013F	 0.32B	 0	 12C	 40	 19	 25
	 4E
	0.18 - 0.52	 2.99E	 0.24B	 0	 15C	 39	 13	 24
	0.58 - 0.76	 1.3E	 0.1B
	0.76 - 1.07	 0.46E	 0.03B	 43C	 43	 7	 7
	1.12 - 1.3	 0.13E	 0.001F
	1.3 - 1.57	 0.03E	 40C	 37	 3	 19
	1.65 - 1.93
	1.98 - 2.13
	2.13 - 2.36
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.18
	0.18 - 0.52
	0.58 - 0.76
	0.76 - 1.07
	1.12 - 1.3
	1.3 - 1.57
	1.65 - 1.93
	1.98 - 2.13
	2.13 - 2.36

	Project Name:	CL
	Project Code:	CL	Site ID:	B339	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_CEC	CEC - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2A1	Air-dry moisture content
	3A_TSS	Electrical conductivity or soluble salts - Total soluble salts %
	4_NR	pH of soil - Not recorded
	5_NR	Water soluble Chloride - Cl(%) - Not recordede
	6Z	Organic carbon (%) - Not recorded
	7_NR	Total nitrogen (%) - Not recorded
	9_NR	Available P (mg/kg) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded