Project Name:	CL
	Project Code:	CL	Site ID:	B562	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Site Information
	Desc. By:	C.H. Thompson	Locality:
	Date Desc.:	12/10/66	Elevation:	 12 metres
	Map Ref.:	Sheet No. : 9544   1:100000	Rainfall:	1632
	Northing/Long.:	153.016666666667	Runoff:	Very slow
	Easting/Lat.:	-26.85	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	Auger boring, 2 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Magnesic Chomosolic Redoxic Hydrosol     	Principal Profile Form:	Dy5.41
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Xanthorrhoea media
	Mid Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.05 m	Dark grey (10YR4/1-Moist); ; Sand (Heavy); Massive grade of structure; Moist; Very weak 
	consistence; Field pH 5.6 (pH meter); Common, fine (1-2mm) roots; Clear change to - 
	A12	0.05 - 0.1 m	Light brownish grey (10YR6/2-Moist); , 7.5YR58, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, 
	Distinct; Sand; Massive grade of structure; Moist; Very weak consistence; Field pH 5.6 (pH 
	meter); Common, fine (1-2mm) roots; 
	A12	0.1 - 0.2 m	Light brownish grey (10YR6/2-Moist); , 7.5YR58, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, 
	Distinct; Sand; Massive grade of structure; Moist; Very weak consistence; Field pH 5.4 (pH 
	meter); Common, fine (1-2mm) roots; Diffuse change to - 
	A21	0.2 - 0.3 m	Light grey (10YR7/2-Moist); , 10YR56, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; Sand;
	 Massive grade of structure; Moist; Very weak consistence; Field pH 5.2 (pH meter); Few, fine 
	(1-2mm) roots; 
	A21	0.3 - 0.35 m	Light grey (10YR7/2-Moist); , 10YR56, 2-10% , 0-5mm, Distinct; , 2-10% , 0-5mm, Distinct; Sand;
	 Massive grade of structure; Moist; Very weak consistence; Field pH 5 (pH meter); Diffuse 
	change to - 
	A22	0.35 - 0.5 m	White (10YR8/1-Moist); ; Sand; Massive grade of structure; Moist; Very weak consistence; 
	Field pH 5.2 (pH meter); Abrupt change to - 
	B11	0.5 - 0.55 m	Light grey (10YR7/1-Moist); , 10YR58, 10-20% , 15-30mm, Prominent; , 10YR48, 10-20% , 15-
	30mm, Prominent; Clayey sand; Weak grade of structure, 100-200 mm, Columnar; Moist; Firm 
	consistence; Field pH 4.9 (pH meter); Gradual change to - 
	B12	0.55 - 0.6 m	Grey (10YR6/1-Moist); , 10YR58, 20-50% , 15-30mm, Prominent; , 10YR66, 20-50% , 15-30mm, 
	Prominent; Sandy clay loam; , Columnar; 20-50 mm, Angular blocky; Moist; Firm consistence; 
	Field pH 4.9 (pH meter); 
	B12	0.6 - 0.75 m	Grey (10YR6/1-Moist); , 10YR58, 20-50% , 15-30mm, Prominent; , 10YR66, 20-50% , 15-30mm, 
	Prominent; Sandy clay loam; , Columnar; 20-50 mm, Angular blocky; Moist; Firm consistence; 
	Field pH 5.2 (pH meter); 

	Project Name:	CL
	Project Code:	CL	Site ID:	B562	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	B12	0.75 - 0.9 m	Grey (10YR6/1-Moist); , 10YR58, 20-50% , 15-30mm, Prominent; , 10YR66, 20-50% , 15-30mm, 
	Prominent; Sandy medium clay; 20-50 mm, Angular blocky; Moist; Firm consistence; Field pH 5 
	(pH meter); Diffuse change to - 
	B21	0.9 - 1.2 m	Light grey (2.5Y7/1-Moist); , 7.5YR56, 20-50% , 15-30mm, Prominent; , 2.5YR48, 20-50% , 15-
	30mm, Prominent; Sandy medium clay (Light); Moderate grade of structure, 20-50 mm, Angular 
	blocky; Moist; Moderately plastic; 0-2%, medium gravelly, 6-20mm, subrounded, Quartz, coarse 
	fragments; Field pH 5.1 (pH meter); Diffuse change to - 
	B22	1.2 - 1.3 m	 (N7/0-Moist); , 10YR58, 20-50% , 15-30mm, Prominent; , 2.5YR36, 20-50% , 15-30mm, 
	Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Angular blocky; Wet; 
	Moderately plastic; 0-2%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; 
	Field pH 5 (pH meter); 
	B22	1.3 - 1.5 m	 (N7/0-Moist); , 10YR58, 20-50% , 15-30mm, Prominent; , 2.5YR36, 20-50% , 15-30mm, 
	Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Angular blocky; Wet; 
	Moderately plastic; 0-2%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; 
	Field pH 4.9 (pH meter); 
	B22	1.5 - 1.6 m	 (N7/0-Moist); , 10YR58, 20-50% , 15-30mm, Prominent; , 2.5YR36, 20-50% , 15-30mm, 
	Prominent; Medium clay; Moderate grade of structure, 5-10 mm, Angular blocky; Wet; 
	Moderately plastic; 0-2%, medium gravelly, 6-20mm, subrounded, Quartz, coarse fragments; 
	Field pH 5 (pH meter); Diffuse change to - 
	B31	1.6 - 1.8 m	White (5Y8/1-Moist); , 10R32, 20-50% , 15-30mm, Prominent; , 10YR56, 20-50% , 15-30mm, 
	Prominent; Medium heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; Wet; 0-
	2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 5 (pH meter); 
	B31	1.8 - 2 m	White (5Y8/1-Moist); , 10R32, 20-50% , 15-30mm, Prominent; , 10YR56, 20-50% , 15-30mm, 
	Prominent; Medium heavy clay; Moderate grade of structure, 20-50 mm, Angular blocky; Wet; 0-
	2%, medium gravelly, 6-20mm, Quartz, coarse fragments; Field pH 4.9 (pH meter); Diffuse 
	change to - 
	B32	2 - 2.1 m	White (5Y8/1-Moist); , 10R32, 20-50% , 15-30mm, Prominent; , 2.5Y76, 20-50% , 15-30mm, 
	Prominent; Heavy clay; Massive grade of structure; Moist; Very firm consistence; Field pH 4.9 
	(pH meter); 
	B32	2.1 - 2.4 m	White (5Y8/1-Moist); , 10R32, 20-50% , 15-30mm, Prominent; , 2.5Y76, 20-50% , 15-30mm, 
	Prominent; Massive grade of structure; Moist; Very firm consistence; Field pH 5 (pH meter); 
	B32	2.4 - 2.7 m	White (5Y8/1-Moist); , 10R32, 20-50% , 15-30mm, Prominent; , 2.5Y76, 20-50% , 15-30mm, 
	Prominent; Massive grade of structure; Moist; Very firm consistence; Field pH 5 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	BEERWAH

	Project Name:	CL
	Project Code:	CL	Site ID:	B562	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.6A	 0.027A	 0.6B	 0.58	 0.03	 0.04	 0.92D
	0.05 - 0.1	5.6A	 0.019A	 0.2B	 0.3	 0.02	 0.06	 0.56D
	0.1 - 0.2	5.4A	 0.014A
	0.2 - 0.3	5.2A	 0.014A
	0.3 - 0.35	5A	 0.019A
	0.35 - 0.5	5.2A	 0.014A	 0.04B	 0.1	 0.02	 0.04	 0.4D
	0.5 - 0.55	4.9A	 0.024A	 0.1B	 0.16	 0.02	 0.04	 0.8D
	0.55 - 0.6	4.9A	 0.027A
	0.6 - 0.75	5.2A	 0.03A	 0.1B	 0.67	 0.02	 0.12	 2.1D
	0.75 - 0.9	5A	 0.03A	 0.05B	 0.84	 0.02	 0.14	 2.8D
	0.9 - 1.2	5.1A	 0.032A	 0.05B	 1.3	 0.02	 0.43	 2.3D
	1.2 - 1.3	5A	 0.038A
	1.3 - 1.5	4.9A	 0.046A	 0.05B	 2.5	 0.03	 0.57	 7.7D
	1.5 - 1.6	5A	 0.043A
	1.6 - 1.8	5A	 0.046A	 0.06B	 2.4	 0.02	 0.51	 6.5D
	1.8 - 2	4.9A	 0.038A
	2 - 2.1	4.9A	 0.03A
	2.1 - 2.4	5A	 0.038A
	2.4 - 2.7	5A	 0.035A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.1A	 2.8A	 0.002A	 0.042B	 0.03A	1.35	 1	 56C	 34	 6	 2
	 2.7B
	0.05 - 0.1	 0.41A	 4A	 0.001A	 0.016B	 0.03A	1.49	 1	 57C	 34	 6	 2
	 1.7B
	0.1 - 0.2	 0.23A	 0.004A	 0.013B	 0.04A	 1	 51C	 38	 6	 3
	0.2 - 0.3	 0.001A	 0.012B	 0.03A	1.64	 1	 53C	 39	 6	 2
	0.3 - 0.35
	0.35 - 0.5	<0A	 0.007B	 0.02A	 1	 43C	 34	 14	 8
	0.5 - 0.55	<0A	 0.005B	 0.03A	1.87	 1	 40C	 37	 13	 11
	0.55 - 0.6
	0.6 - 0.75	 0.002A	 0.006B	 0.04A	 1	 39C	 34	 8	 18
	0.75 - 0.9	 0.002A	 0.006B	 0.05A	 1	 39C	 30	 7	 22
	0.9 - 1.2	 0.001A	 0.008B	 0.06A	1.67	 1	 37C	 25	 8	 29
	1.2 - 1.3
	1.3 - 1.5	 0.003A	 0.009B	 0.21A	 1	 26C	 14	 12	 49
	1.5 - 1.6
	1.6 - 1.8	 0.001A	 0.008B	 0.22A	 1	 28C	 19	 12	 42
	1.8 - 2
	2 - 2.1
	2.1 - 2.4
	2.4 - 2.7	 1	 32C	 11	 13	 46
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05	0.15F	0.05H

	Project Name:	CL
	Project Code:	CL	Site ID:	B562	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	0.05 - 0.1	0.18F	0.04H
	0.1 - 0.2
	0.2 - 0.3	0.16F	0.04H
	0.3 - 0.35
	0.35 - 0.5
	0.5 - 0.55	0.27F	0.19H
	0.55 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1.2	0.34F	0.27H
	1.2 - 1.3
	1.3 - 1.5
	1.5 - 1.6
	1.6 - 1.8
	1.8 - 2
	2 - 2.1
	2.1 - 2.4
	2.4 - 2.7

	Project Name:	CL
	Project Code:	CL	Site ID:	B562	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (QLD)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1	Organic carbon - Walkley and Black
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A1	Bulk density - g/cm3
	P3B3VLe004	0.04 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe01	0.1 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe03	0.3 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	suction plate
	P3B3VLe06	0.6 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe15	15 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe2	2 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate
	P3B3VLe7	7 BAR Moisture m3/m3 - Volumetric using undisturbed 60mm diameter and 34mm height core on 
	pressure plate